Patch-ID# 118979-02

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************

Keywords: sun ray update patch security
Synopsis: Sun Ray Core Services version 3.0 Patch Update
Date: Dec/13/2005


Install Requirements: Reboot after installation, an alternative may be in Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: Sun Ray Core Services

Unbundled Release: 3.0

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4818663 4950642 5092486 6189847 6190711 6199882 6203451 6203630 6205407 6207996 6211438 6212211 6213562 6218260 6223797 6225835 6226501 6228580 6230062 6230157 6238984 6240497 6242160 6245587 6253785 6259230 6263842 6266420 6275880 6278092 6296051 6296978 6300477 6309580 6309587 6309589 6310241 6310253 6310254 6311482 6319180 6325171 6346040

Changes incorporated in this version: 6319180 6238984 6263842 6266420 6278092 6275880 6259230 6296978 6325171 6346040 4950642 6300477 6309587 6309589 6309580 6310241 6310253 6310254 6311482 4818663 6296051

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/etc/init.d/utacleanup
/etc/opt/SUNWut/smartcard/Belgian-eID.cfg
/etc/opt/SUNWut/smartcard/Cryptoflex.cfg
/etc/opt/SUNWut/smartcard/DatakeyModel330SafeNet.cfg
/etc/opt/SUNWut/smartcard/FCU.cfg
/etc/opt/SUNWut/smartcard/ORGA-Micardo.cfg
/etc/opt/SUNWut/smartcard/probe_order.conf
/opt/SUNWut/bin/utwho
/opt/SUNWut/bin/utxconfig
/opt/SUNWut/cgi-bin/ade
/opt/SUNWut/cgi-bin/admincgi
/opt/SUNWut/cgi-bin/copyright
/opt/SUNWut/cgi-bin/crypto
/opt/SUNWut/cgi-bin/desktop
/opt/SUNWut/cgi-bin/error
/opt/SUNWut/cgi-bin/gstatus
/opt/SUNWut/cgi-bin/log
/opt/SUNWut/cgi-bin/main
/opt/SUNWut/cgi-bin/mhstatus
/opt/SUNWut/cgi-bin/nav
/opt/SUNWut/cgi-bin/smartcard
/opt/SUNWut/cgi-bin/start
/opt/SUNWut/cgi-bin/status
/opt/SUNWut/cgi-bin/usb
/opt/SUNWut/cgi-bin/user
/opt/SUNWut/cgi-bin/usersession
/opt/SUNWut/lib/firmware/CoronaP1
/opt/SUNWut/lib/firmware/CoronaP2
/opt/SUNWut/lib/firmware/CoronaP3
/opt/SUNWut/lib/firmware/CoronaP4
/opt/SUNWut/lib/firmware/CoronaP5
/opt/SUNWut/lib/firmware/CoronaP6
/opt/SUNWut/lib/firmware/CoronaP7
/opt/SUNWut/lib/guloginGUI
/opt/SUNWut/lib/libutjadmin.so
/opt/SUNWut/lib/libutsmon.so.1
/opt/SUNWut/lib/locale/html/main/replace.html
/opt/SUNWut/lib/locale/html/nav.html
/opt/SUNWut/lib/locale/html/start/start.html
/opt/SUNWut/lib/nscloginGUI
/opt/SUNWut/lib/scloginGUI
/opt/SUNWut/lib/utdomount
/opt/SUNWut/lib/utparalleld
/opt/SUNWut/lib/utseriald
/opt/SUNWut/lib/utstoraged
/opt/SUNWut/lib/utxinit
/opt/SUNWut/sbin/utcard
/opt/SUNWut/sbin/utdesktop
/opt/SUNWut/sbin/utfwadm
/opt/SUNWut/sbin/utfwload
/opt/SUNWut/sbin/utmhadm
/opt/SUNWut/sbin/utuser
/usr/dt/config/Xsession.d/0100.SUNWut
/usr/kernel/drv/sparcv9/utdisk
/usr/kernel/drv/sparcv9/utdiskctl
/usr/kernel/drv/utdisk
/usr/kernel/drv/utdiskctl
/usr/openwin/server/modules/ddxSUNWsunray.so.1

Problem Description:

6319180 utxconfig is insufficently paranoid
6238984 utseriald dumps core after resetting the DTU connected with serial adapter
6263842 Session is stuck at the grey screen sometimes
6266420 SRSS 3.0 USB printing don't work on Solaris 9 (9/04) and JavaDS 2 (utparalleld problem?)
6278092 Sun Ray doesn't print with HP Laserjet 1320 attached via USB to the Sun Ray
6275880 utfwadm fails on non-english locales with "Error: Improper firmware file"
6259230 New Quatech SSU-100 devices (P/N 990-0044-01D) don't work on Sun Rays
6296978 horizontal dotted lines are displayed as solid lines on FrameMaker 7.1 with SRSS 3.0
6325171 ndbm database corruption causes utdesktop and authd to core dump.
6346040 Update smartcard config files to work with new versions of cards
4950642 Sun Ray web GUI should reduce volume of logfile output
6300477 Unlocalized messages for "Add user" in AdminGUI
6309587 Error message page is observed during add user of admin GUI using token reader
6309589 Blank page is observed when deleting/updating user from admin GUI
6309580 Trying to restart services from Admin GUI gives error.
6310241 Viewing added smartcards through "view" link of admin GUI gives error page
6310253 Error page is displayed when tried to view the multihead group from Admin GUI
6310254 View by server gives error page from admin GUI in a HA group
6311482 Restart of Sun Ray services from Admin GUI using netscape7 is not working as expected
4818663 utxlock should not be enabled for CAM sessions
6296051 some filesystems on Sun Ray disks are mounted with setuid enabled
 
(from 118979-01)
6218260 Scroll wheel on Genius NetScroll and PowerScroll mice is not recognised
6213562 Scroll wheel on Logitech M-BJ58 mouse is not recognised
6226501 Scroll wheel on Logitech M-BT85 Click! optical wheel mice is not recognised
6228580 Scroll wheel on Fujitsu PID==0x1001 mouse is not recognised
6199882 DTU rx buffer management deadlocks if input queue grows too large
6203630 USB printing fails with some USB printers
6212211 SunRay The position of the mouse pointer is random on xinerama displays
6190711 Mouse cursor is lost in Xinerama when video is played in enlarged realplayer
5092486 Mouse pointer tracking is not stable under stress in multihead
6223797 Setting router equal to Sun Ray's IP address should invoke proxy ARP
6203451 utwho/utfwload fail in en_US.ISO8859-1 locale because final join doesn't work
6240497 SRSS 3.0 firmware ignores DHCP option 49 when DHCP_INFORM is not received.
6230062 Sun Ray 170 should support multiple resolutions
6225835 yuv transformation underflows on black pixels
6242160 Xsun's footprint quickly soares to over 2GB when Cadence on sunray is used and then it crashes
6253785 T=1 smartcard works on first insertion but not again unless DTU is power cycled or Ctrl+Moon.
6211438 When utselecting with SRSS 3.0, the target system loses control of keyboard and sometimes mouse
6245587 utcard for not being able to remove partially  configured card.
6189847 With "pam_sunray.so" in the PAM stack kerberos credential generation fails
6205407 system panics when utdisk module is unloaded after utdiskctl module is unloaded
6207996 mass storage kernel drivers incorrectly assume that attach(9E) occurs before open(9E)
6230157 utstorage message queue handling is broken

Patch Installation Instructions:
-------------------------------- 
For Solaris 8 and later release, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.  Any other
special or non-generic installation instructions should be described below
as special instructions.  The following example installs a patch to a
standalone machine:
 
        example# patchadd /var/spool/patch/<patchid-rev>
 
The following example removes a patch from a standalone system:
 
        example# patchrm <patchid-rev>
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
NOTE: This patch is for the Sun Ray Core Services 3.0 component that is
part of Sun Ray Server Software 3.0.
 
NOTE: This SRSS patch does not support Live Upgrade.  Please do not
install this patch via live upgrade.
 
NOTE: The DTU firmware delivered in this patch has the following version
identification string
 
    3.0_118979-02_2005.11.28.11.24
 
Required Patches
----------------
 
Warnings & Errors
-----------------
** WARNING: This patch should only be applied to systems which have
	    Sun Ray Server Software 3.0 fully installed.  Do not attempt
	    to add this patch to the UFS image to be applied as part of
	    the install process **
 
Detailed Steps
--------------
 
1. Suppress firmware downloads
 
	If the server being patched is not a member of a Sun Ray
	failover group you should skip this step.
 
	If the server being patched is a member of a Sun Ray failover
	group then this step is optional but is strongly recommended.
 
	At Patch Installation
	---------------------
 
	    Before adding this patch to servers configured into a Sun
	    Ray failover group we advise that you disable Sun Ray
	    firmware delivery from all unpatched hosts in the failover
	    group.  On each host in the group:
 
		For each of the dedicated network interconnects:
 
		    $ /opt/SUNWut/sbin/utfwadm -a -D -n <intf>
 
		For each of the shared subnetwork interconnects:
 
		    $ /opt/SUNWut/sbin/utfwadm -a -D -N <subnetwork>
 
	    Do this only one time, before adding this patch to any
	    server in the group.
 
	    The purpose of this step is to prevent unpatched servers
	    from offering old firmware to Sun Ray appliances.
 
	At Patch Removal
	----------------
 
	    Before removing this patch from servers configured into a
	    Sun Ray failover group we advise that you disable firmware
	    delivery from any hosts in the failover group that have
	    this patch installed.  On each already-patched host in the
	    group:
 
		For each of the dedicated network interconnects:
 
		    $ /opt/SUNWut/sbin/utfwadm -a -D -n <intf>
 
		For each of the shared subnetwork interconnects:
 
		    $ /opt/SUNWut/sbin/utfwadm -a -D -N <subnetwork>
 
	    Do this only one time, before removing this patch from any
	    of the already-patched servers in the group.
 
	    The purpose of this step is to prevent already-patched
	    servers from offering new firmware to Sun Ray appliances.
 
	    If this patch is being removed from a Sun Ray failover group
	    then omitting this step may result in increased restart
	    times for your Sun Ray appliances.  (A mixture of patched
	    and unpatched servers advertising conflicting firmware
	    versions may cause the appliance to download new firmware
	    each time it restarts.  The appliance automatically
	    restarts itself after downloading fresh firmware so its
	    overall restart cycle is longer in that case.  The
	    appliance may restart itself several times before
	    establishing or reconnecting to a session.)  The Sun Ray
	    restart time will return to normal once the patch has been
	    removed from all servers in the failover group.
 
 
2. Stopping Sun Ray services and login sessions
 
	Before the addition or removal of this patch to a Sun Ray server
	all users should be logged out of their Sun Ray sessions.
 
	Stop the Sun Ray services using the following commands:
 
                $ /etc/init.d/utstorage stop
                $ /etc/init.d/utsvc stop
 
	These commands will terminate any Sun Ray sessions that were not
	already logged out.
 
	Next, use the instructions outlined above in the section
	"Patch Installation Instructions" for the addition or removal
	of this patch.
 
	Adding the patch automatically prepares the server to advertise
	new firmware to your Sun Ray appliances.
 
	Removing the patch automatically prepares the server to revert to
	advertising pre-patch firmware to your Sun Ray appliances.
 
3. Rebooting the Sun Ray server
 
	The Sun Ray server must be rebooted after the addition or removal
	of the patch.
 
4. Enable firmware downloads
 
	After the addition or removal of this patch on all Sun Ray
	servers in a failover group, enable firmware downloads
	using one of the following methods:
 
	1) If all Sun Ray server in the failover group provides firmware
	   downloads run this command on one of the servers:
 
		$ /opt/SUNWut/sbin/utfwsync
 
	   After which the Sun Ray DTU's will reboot themselves and load
	   the new firmware.
 
	2) If only some of the Sun Ray servers in the failover group provide
	   firmware downloads to the DTU's, run the following command
	   on the servers that do provide firmware:
 
	   For each in dedicated network interconnects:
 
		$ /opt/SUNWut/sbin/utfwadm -a -A -n <intf>
 
	   For each in shared subnetwork interconnects:
 
		$ /opt/SUNWut/sbin/utfwadm -a -A -N <subnetwork>
 
	   Then restart services on all servers in the failover group by
	   executing the following command on a server in the group:
 
		$ /opt/SUNWut/sbin/utfwsync -d

README -- Last modified date:  Tuesday, December 13, 2005

