Enterprise Servers

V1280 Server

12 USIII CPU's

E2900

V1280

E2900 Server

12 USIV CPU's

F6800

F4800

Sun Rack 900

E4900

E6900

F6800 Server

Capacity for:

24 USIII CPU's

374 GB memory

4 Domains

F4800 Server

Capacity for:

12 USIII CPU's

192 GB memory

2 Domains

E4900 Server

Capacity for:

12 USIV CPU's

192 GB memory

2 Domains

E6900 Server

Capacity for:

24 USIV CPU's

374 GB memory

4 Domains

V1280 Server Detail

V1280 Server

12 USIII CPU's - 1.2 GHz (1.05 GHz available)

24 GB memory (96 GB max)

2 internal 73 GB LVD SCSI disks

DVD

DDS-4 Tape Option

6 PCI Cards - 1x 66 MHz, 5x 33 MHz

2x 10/100/1000 Cat-5 Ethernet

2N Power & Fans.

4 Power Cords

12 Rack Units high

Included Rack Mount Kit works with

Sun 900 Rack & Sun 72” Cabinet

V1280 Server

LVD SCSI VHDCI

DVD

Space

for Disk

PCI 0 – 33 MHz Slot

Standby System Controller

Ethernet 10/100 RJ45

Space

for

CPU

Memory

Board

L2 Address Repeater Switch

L2 Address Repeater Switch

Alarms Port DB15

Space for

DDS-4 Tape

PCI 1 – 33 MHz Slot

PCI 2 – 33 MHz Slot

PCI 3 – 33 MHz Slot

PCI 4 – 33 MHz Slot

PCI 5 – 66 MHz Slot

System Config Card

10/100/1000 Cat-5 Enet RJ45

Power Supply 0

Source

B

Serial RJ45

Power Supply 1

Power Supply 2

Power Supply 3

SCSI

Source

A

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Memory

Board

Space

for

CPU

Memory

Board

Space

for Disk

73 GB

LVD Disk

73 GB

LVD Disk

CPU / Memory

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

CPU / Memory

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

CPU / Memory

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

1.2 GHz

USIII

1 GB

1 GB

E2900 Server Detail

E2900 Server

12 USIV CPU's - 1.2 GHz (1.05 GHz available)

48 GB memory (96 GB max)

2 internal 73 GB LVD SCSI disks

DVD

DDS-4 Tape Option

6 PCI Cards - 1x 66 MHz, 5x 33 MHz

2x 10/100/1000 Cat-5 Ethernet

2N Power & Fans.

4 Power Cords

12 Rack Units high

Included Rack Mount Kit works with

Sun 900 Rack & Sun 72” Cabinet

E2900 Server

LVD SCSI VHDCI

DVD

Space

for Disk

PCI 0 – 33 MHz Slot

Standby System Controller

Version 2

Ethernet 10/100 RJ45

Space

for

CPU

Memory

Board

L2 Address Repeater Switch

L2 Address Repeater Switch

Alarms Port DB15

Space for

DDS-4 Tape

PCI 1 – 33 MHz Slot

PCI 2 – 33 MHz Slot

PCI 3 – 33 MHz Slot

PCI 4 – 33 MHz Slot

PCI 5 – 66 MHz Slot

System Config Card

10/100/1000 Cat-5 Enet RJ45

Power Supply 0

Source

B

Serial RJ45

Power Supply 1

Power Supply 2

Power Supply 3

SCSI

Source

A

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Memory

Board

Space

for

CPU

Memory

Board

Space

for Disk

CPU / Memory

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

CPU / Memory

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

CPU / Memory

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

73 GB

LVD Disk

73 GB

LVD Disk

F4800 Server Detail

2 D240 Media Trays

Each with: DVD

2 x 73 GB disks

DDS-4 Tape Drive

F4800 Server

12 USIII CPU's - 1.2 GHz (1.05 GHz available)

48 GB Memory (96 GB max)

Domain Configuration

Label	Function	Segment	CPU's	Memory

A	Production	0	4	8 GB

B	(not available)

C*	Staging	1	8	16 GB

D*	(not available)

* Segmenting the system enables use of these

Domains

NOTE: Each Domain requires at least one

CPU / Memory Board and one I/O Assembly.

F4800

D240

D240

Fan Tray

L2 Address Repeater Switch

A

A

C

C

Fan Tray

Fan Tray

Power Supply

Power Supply

Power Supply

L2 Address Repeater Switch

A

C

C

66

33

33

33

66

33

33

33

Top I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

Bottom I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Serial A/B DB25

100/10 Ethernet RJ45

System Controller

Serial A/B DB25

100/10 Ethernet RJ45

System Controller

Space for

Uniboard

Space for

Uniboard

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Space for

Uniboard

Space for

Uniboard

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Space for

Uniboard

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

E4900 Server Detail

2 D240 Media Trays

Each with: DVD

2 x 73 GB disks

DDS-4 Tape Drive

E4900 Server

12 USIV CPU's - 1.2 GHz (1.05 GHz available)

48 GB Memory (96 GB max)

Domain Configuration

Label	Function	Segment	CPU's	Memory

A	Production	0	4	8 GB

B	(not available)

C*	Staging	1	8	16 GB

D*	(not available)

* Segmenting the system enables use of these

Domains

NOTE: Each Domain requires at least one

CPU / Memory Board and one I/O Assembly.

F4800

D240

D240

Fan Tray

L2 Address Repeater Switch

A

A

C

C

Fan Tray

Fan Tray

Power Supply

Power Supply

Power Supply

L2 Address Repeater Switch

A

C

C

66

33

33

33

66

33

33

33

Top I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

Bottom I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Serial A/B DB25

100/10 Ethernet RJ45

System Controller

Version 2

Serial A/B DB25

100/10 Ethernet RJ45

System Controller

Version 2

Space for

Uniboard

Space for

Uniboard

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Space for

Uniboard

Space for

Uniboard

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Space for

Uniboard

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Domain Configuration

Label	Function	Segment	CPU's	Memory

A	Production	0	12	48 GB

B	(available)	0

C*	Staging	1	12	48 GB

D*	(available)	1

* Segmenting the system enables use of these

Domains

NOTE: Each Domain requires at least one

CPU / Memory Board and one I/O Assembly.

2 D240 Media Trays

Each with: DVD

2 x 73 GB disks

DDS-4 Tape Drive

F6800 Server

24 USIII CPU's - 1.2 GHz

(1.05 GHz available)

96 GB Memory (192 GB max)

F6800 Server Detail

E6800

D240

D240

PS

L2 Address Repeater Switch

L2 Address Repeater Switch

L2 Address Repeater Switch

L2 Address Repeater Switch

PS

PS

PS

PS

PS

A

A

A

C

A

A

C

A

C

C

C

C

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Left I/O Assy - PCI

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Bottom Right I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Right I/O Assy - PCI

66

33

33

33

66

33

33

33

Bottom Left I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

DB25 Serial A/B

RJ45 100/10 Ethernet

System Controller

DB25 Serial A/B

RJ45 100/10 Ethernet

System Controller

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

Domain Configuration

Label	Function	Segment	CPU's	Memory

A	Production	0	12	48 GB

B	(available)	0

C*	Staging	1	12	48 GB

D*	(available)	1

* Segmenting the system enables use of these

Domains

NOTE: Each Domain requires at least one

CPU / Memory Board and one I/O Assembly.

2 D240 Media Trays

Each with: DVD

2 x 73 GB disks

DDS-4 Tape Drive

E6900 Server

24 USIV CPU's - 1.2 GHz

(1.05 GHz available)

96 GB Memory (192 GB max)

E6900 Server Detail

F6900

D240

D240

PS

L2 Address Repeater Switch

L2 Address Repeater Switch

L2 Address Repeater Switch

L2 Address Repeater Switch

PS

PS

PS

PS

PS

A

A

A

C

A

A

C

A

C

C

C

C

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Left I/O Assy - PCI

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Bottom Right I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Right I/O Assy - PCI

66

33

33

33

66

33

33

33

Bottom Left I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

DB25 Serial A/B

RJ45 100/10 Ethernet

System Controller

Version 2

DB25 Serial A/B

RJ45 100/10 Ethernet

System Controller

Version 2

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

Domain A: Production

Domain A: Production

A

A

A

A

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Bottom Right I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Right I/O Assy - PCI

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

6120 2x2

4 TB Disk, 2 GB cache

A

B

6120 Disk Array

Space for RAID Controller

RJ45 Serial

RJ45 Enet

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146

H/W RAID Controller

with 1 GB Cache

LC FC

A

B

Space for RAID Controller

RJ45 Serial

RJ45 Enet

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146

H/W RAID Controller

with 1 GB Cache

LC FC

146

146

LC-LC fiber

5 meters

incl w/ 6120

LC-LC fiber

5 meters

incl w/ 6120

SG-PCI1FC-QF2 2Gb FC

LC

SG-PCI1FC-QF2 2Gb FC

LC

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

73 GB

73 GB

73 GB

DVD

HD68

HD68

HD68

HD68

D240

VHDCI-HD68

4 meters

X3830A

X3830A

Site Plan

2 ft x 2 ft

Tile

E6900

Power cords are

NEMA L6-30P

200/240 VAC

Single Phase

30 amps per RTU

Sun Fire

Cabinet

Power cords are

NEMA L6-30P

200/240 VAC

Single Phase

30 amps per RTU

Sun Fire

Cabinet

24" Width

37" Depth

75" Height

Clearances:

48" Front

36" Back

R

T

S

R

T

S

RTU

Each RTU can support 2 RTS's.

Only one RTS will be utilized at a time.

The intent of the second RTS is to provide

a connection to a second power source.

If a second power source is not available,

then use only one RTS in each RTU.

Space

for

RTU

R

T

S

R

T

S

RTU

R

T

S

R

T

S

RTU

F6800

Cabinet

24" Width

57" Depth

75" Height

Clearances:

48" Front

36" Back

Sun Rack 900

Power cords are

NEMA L6-20P

200/240 VAC

Single Phase

16 amps each

Sun Rack 900

23.5" Width

35.4" Depth

74" Height

Clearances:

48" Front

36" Back

Power Distribution Sys:

12 outlets per external

power cord

20 internal cords included

24 outlets

24 outlets

Front Door Option

Uniboards

USIII

1.2 GHz

US IV

1.05 GHz

USIV

1.2 GHz

USIII

1.05 GHz

N/A*

N/A*

2 GB

N/A*

N/A*

2 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

US III

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.05

GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.05

GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.05

GHz

USIII

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

N/A*

N/A*

2 GB

N/A*

N/A*

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

US III

PCI Cards & Cables

SCSI Cables

X979A

X973A

SC-SC fibre

2 meters

X978A

HD68 - HD68

SC - SC Fibre

X9715A

VHDCI - HD68

VHDCI - VHDCI

Fibre Cables

SC - LC Fibre

LC / LC Fibre

X1138A

VHDCI-VHDCI

2 meters

X3830B

VHDCI-VHDCI

4 meters

X3831B

VHDCI-VHDCI

10 meters

X1136A

VHDCI-VHDCI

0.8 meter

X3810A

X1132A

VHDCI-HD68

0.8 meter

X1134A

HD68-HD68

0.8 meter

X1139A

HD68-HD68

2 meters

HD68-HD68

4 meters

HD68-HD68

12 meters

X3832A

VHDCI-HD68

2 meters

X3830A

VHDCI-HD68

4 meters

X3831A

VHDCI-HD68

10 meters

SC-SC fibre

5 meters

SC-SC fibre

15 meters

X9722A

SC-LC fibre

2 meters

X9721A

SC-LC fibre

0.4 meter

X9723A

SC-LC fibre

5 meters

X9724A

SC-LC fibre

15 meters

X9735A

SC-LC fibre

25 meters

X9737A

SC-LC fibre

50 meters

X9732A

LC-LC fibre

2 meters

X9733A

LC-LC fibre

5 meters

X9734A

LC-LC fibre

15 meters

X9736A

LC-LC fibre

25 meters

X9738A

LC-LC fibre

50 meters

X1137A

VHDCI-VHDCI

1.2 meters

1034A Quad 100 Enet RJ45's

66/33 MHz PCI Cards

33 MHz PCI Cards

PCI Cards

1155A High Speed Serial 2.0

1071A HIPPI/P 1.1

2156A Serial Async 3.0

1151A Gb Enet

MMF

1150A 1000/100/10 Enet

RJ45

6799A Gb FC

SC

6727A Dual Gb FC

SC

SC

SG-XPCI1FC-QF2 2Gb FC

LC

SG-XPCI2FC-QF2 2Gb FC

LC

LC

6758A Dual LVD SCSI

VHDCI

VHDCI

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

6540A UltraSCSI

VHDCI

VHDCI

6541A UltraSCSI Diff

VHDCI

VHDCI

1157A ATM 155 4.0

MMF

X9739A

SC-SC fibre

100 meters

Was 6767A

Was 6768A

SG-XPCI1FC-JF2 JNI 2Gb

LC

Last Order Data: 4/16/04

Last Order Data: 4/16/04

3151A Gb Enet

MMF

3150A 1000/100/10 Enet

RJ45

SG-XPCI2FC-JF2 JNI 2Gb

LC

LC

1074A SCI cluster

Last Order Data: 6/09/04

Last Order Data: 8/24/04

2222A

10/100 Enet Dual RJ45's

LVD SCSI Dual VHDCI's

Full Length: does not fit into V2900/V1280

4444A 10/100/1000 Enet RJ45's

Tom Meier

2000-03-25T11:55:10