Sun Fire 12K, 15K, E20K & E25K

Sun Fire 15K Server

Capacity for:

106 USIII CPU's

576 GB memory

18 domains

Sun Fire 12K Server

Capacity for:

52 USIII CPU's

288 GB memory

9 domains

12K

Sun Fire E20K Server

Capacity for:

36 USIV CPU's

288 GB memory

9 domains

Sun Fire E25K Server

Capacity for:

72 USIV CPU's

576 GB memory

18 domains

15K

E25K

E20K

Boot Disks

Mirrored S1's

Racking

Sun Rack 900

Sun Fire E25K Server

72 USIV CPU's

576 GB memory

18 domains

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

Sun Fire 12K Server

F12K Back

F12K Front

Domain	Use	CPUs	Memory	Usable Disk

A	Production	12	48 GB	290 GB*

B	Production	8	32 GB	608 GB*

C	Production	8	32 GB	524 GB*

D	Production	8	32 GB	276 GB*

Total	36	144 GB	1.8 TB

*has mirror of same size for backup

8

7

6

5

4

3

2

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

1

0

17

16

15

14

13

12

11

10

9

Sys Control #1

Sys Control #2

System

Controller

Board

Serial DB9

Ethernet RJ45

CPU

Card

Ethernet RJ45

System

Controller

Board

RJ45 Ethernet

DB9 Serial

CPU

Card

RJ45 Ethernet

Slots 9-17 are disabled.

Upgrade is available to enable.

Domain A

Domain B

Domain C

Domain D

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

Sun Fire 15K Server

Domain	Use	CPUs	Memory	Usable Disk

A	Production	12	48 GB	290 GB*

B	Production	8	32 GB	608 GB*

C	Production	8	32 GB	524 GB*

D	Production	8	32 GB	276 GB*

E	Production	8	32 GB	55 GB*

*has mirror of same size for backup

F15K Back

Domain	Use	CPUs	Memory	Usable Disk

F	Test	4	16 GB	276 GB

G	Dev	4	16 GB	220 GB

H	B Test & Dev	4	16 GB	608 GB

I	App Rel Testing	16	48 GB	939 GB

Available: 2867 GB

Total	72	288 GB	6.6 TB

F15K Front

8

7

6

5

4

3

2

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

1

0

17

16

15

14

13

12

11

10

9

Sys Control #1

Sys Control #2

System

Controller

Board

Serial DB9

Ethernet RJ45

CPU

Card

Ethernet RJ45

System

Controller

Board

RJ45 Ethernet

DB9 Serial

CPU

Card

RJ45 Ethernet

Domain A

Domain B

Domain C

Domain D

Domain E

Domain F

Domain G

Domain H

Domain I

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

Uniboard

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

2 GB

2 GB

1.2

GHz

USIII

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

Sun Fire E20K Server

E20K Back

Domain	Use	CPUs	Memory	Usable Disk

A	Production	12	48 GB	290 GB*

B	Production	8	32 GB	608 GB*

C	Production	8	32 GB	524 GB*

D	Production	8	32 GB	276 GB*

Total	36	144 GB	1.8 TB

*has mirror of same size for backup

8

7

6

5

4

3

2

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

1

0

17

16

15

14

13

12

11

10

9

Sys Control #1

Sys Control #2

System

Controller

Board

Serial DB9

Ethernet RJ45

CPU

Card

Ethernet RJ45

System

Controller

Board

RJ45 Ethernet

DB9 Serial

CPU

Card

RJ45 Ethernet

Slots 9-17 are disabled.

Upgrade is available to enable.

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

E20K Front

Domain A

Domain B

Domain C

Domain D

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

Sun Fire E25K Server

Domain	Use	CPUs	Memory	Usable Disk

A	Production	12	48 GB	290 GB*

B	Production	8	32 GB	608 GB*

C	Production	8	32 GB	524 GB*

D	Production	8	32 GB	276 GB*

E	Production	8	32 GB	55 GB*

*has mirror of same size for backup

E25K Back

Domain	Use	CPUs	Memory	Usable Disk

F	Test	4	16 GB	276 GB

G	Dev	4	16 GB	220 GB

H	B Test & Dev	4	16 GB	608 GB

I	App Rel Testing	16	48 GB	939 GB

Available: 2867 GB

Total	72	288 GB	6.6 TB

E25K Front

8

7

6

5

4

3

2

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

1

0

17

16

15

14

13

12

11

10

9

Sys Control #1

Sys Control #2

System

Controller

Board

Serial DB9

Ethernet RJ45

CPU

Card

Ethernet RJ45

System

Controller

Board

RJ45 Ethernet

DB9 Serial

CPU

Card

RJ45 Ethernet

Domain A

Domain B

Domain C

Domain D

Domain E

Domain F

Domain G

Domain H

Domain I

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

Uniboard

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

2 GB

2 GB

1.05

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

4422A

3150A

SG-PCI1FC-QF2

0

S1: Boot Disks

VHDCI-HD68

10 meters

VHDCI-HD68

10 meters

X3831A

X3831A

S1: Boot Disks Mirror

StorEdge 9980

X9734A

LC-LC fibre

15 meters

LC-LC fibre

15 meters

Typical Domain

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

2

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

HD68

HD68

36 GB

36 GB

36 GB

HD68

HD68

36 GB

36 GB

36 GB

66 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66

66

33

66

66 MHz PCI Slot

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

3150A 1000/100/10 Enet

RJ45

66 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66

66

33

66

66 MHz PCI Slot

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

3150A 1000/100/10 Enet

RJ45

SG-XPCI1FC-JF2 JNI 2Gb

LC

SG-XPCI1FC-JF2 JNI 2Gb

LC

McData

Switch

McData

Switch

X9734A

66 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66

66

33

66

66 MHz PCI Slot

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

3150A 1000/100/10 Enet

RJ45

SG-XPCI1FC-JF2 JNI 2Gb

LC

Site Plan

2 ft x 2 ft

Tile

Sun Fire 15K

33.25" Width

65" Depth

75" Height

Clearances:

36" Front

36" Back

12K

15K

E20k

or

E25K

Power cords are

NEMA #L6-30P

200/240 VAC

Single Phase

24 amps each

Sun StorEdge

SE9980

Controller

Frame

70.5" Cabinet

29.5" Width

31.5" Depth

70.5" Height

Clearances:

31.5" Front

31.5 " Back

Sun StorEdge

SE9980

Disk Array

Frame

70.5" Cabinet

23.6" Width

31.5" Depth

70.5" Height

Clearances:

31.5" Front

31.5 " Back

Sun StorEdge

SE9980

Disk Array

Frame

70.5" Cabinet

23.6" Width

31.5" Depth

70.5" Height

Clearances:

31.5" Front

31.5 " Back

70.5" Cabinet

23.6" Width

31.5" Depth

70.5" Height

Clearances:

31.5" Front

31.5 " Back

SE 9980 Power

Single-Phase:

Power cords are

RussellStol 9P53U2

200/208/230 VAC

50 Amps

3-Phase 60Hz:

Power cords are

Russell Stol RS460PGW

200/208/230 VAC

30 Amp

NOTE: If three phase

is used, then power

for the controller

frame is supplied by

the disk frame.

Sun Rack 900

Power cords are

NEMA L6-20P

200/240 VAC

Single Phase

16 amps each

Sun Rack 900

23.5" Width

35.4" Depth

74" Height

Clearances:

48" Front

36" Back

Power Distribution Sys:

12 outlets per external

power cord

20 internal cords included

24 outlets

24 outlets

Front Door Option

Uniboards

USIII

1.2 GHz

US IV

1.05 GHz

USIV

1.2 GHz

USIII

1.05 GHz

N/A*

N/A*

2 GB

N/A*

N/A*

2 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

US III

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.05

GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.05

GHz

USIII

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

1.2 GHz

USIII

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

USIII

1.2 GHz

USIII

1.05

GHz

USIII

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIII

1.05

GHz

USIII

1.05

GHz

USIII

N/A*

N/A*

2 GB

N/A*

N/A*

2 GB

Uniboard

1.2 GHz

USIII

1.2 GHz

US III

Parts

SCSI Cables

X979A

X973A

SC-SC fibre

2 meters

X978A

HD68 - HD68

SC - SC Fibre

X9715A

VHDCI - HD68

VHDCI - VHDCI

Fibre Cables

SC - LC Fibre

LC / LC Fibre

X1138A

VHDCI-VHDCI

2 meters

X3830B

VHDCI-VHDCI

4 meters

X3831B

VHDCI-VHDCI

10 meters

X1136A

VHDCI-VHDCI

0.8 meter

X3810A

X1132A

VHDCI-HD68

0.8 meter

X1134A

HD68-HD68

0.8 meter

X1139A

HD68-HD68

2 meters

HD68-HD68

4 meters

HD68-HD68

12 meters

X3832A

VHDCI-HD68

2 meters

X3830A

VHDCI-HD68

4 meters

X3831A

VHDCI-HD68

10 meters

SC-SC fibre

5 meters

SC-SC fibre

15 meters

X9722A

SC-LC fibre

2 meters

X9721A

SC-LC fibre

0.4 meter

X9723A

SC-LC fibre

5 meters

X9724A

SC-LC fibre

15 meters

X9735A

SC-LC fibre

25 meters

X9737A

SC-LC fibre

50 meters

X9732A

LC-LC fibre

2 meters

X9733A

LC-LC fibre

5 meters

X9734A

LC-LC fibre

15 meters

X9736A

LC-LC fibre

25 meters

X9738A

LC-LC fibre

50 meters

X1137A

VHDCI-VHDCI

1.2 meters

X9739A

SC-SC fibre

100 meters

Parts

1034A Quad 100 Enet RJ45's

66/33 MHz PCI Cards

33 MHz PCI Cards

PCI Cards

1155A High Speed Serial 2.0

1071A HIPPI/P 1.1

2156A Serial Async 3.0

6799A Gb FC

SC

6727A Dual Gb FC

SC

SC

SG-XPCI1FC-QF2 2Gb FC

LC

SG-XPCI2FC-QF2 2Gb FC

LC

LC

6758A Dual LVD SCSI

VHDCI

VHDCI

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

6540A UltraSCSI

VHDCI

VHDCI

6541A UltraSCSI Diff

VHDCI

VHDCI

1157A ATM 155 4.0

MMF

Was 6767A

Was 6768A

SG-XPCI1FC-JF2 JNI 2Gb

LC

3151A Gb Enet

MMF

3150A 1000/100/10 Enet

RJ45

SG-XPCI2FC-JF2 JNI 2Gb

LC

LC

1074A SCI cluster

Last Order Data: 6/09/04

Last Order Data: 8/24/04

2222A

10/100 Enet Dual RJ45's

LVD SCSI Dual VHDCI's

Full Length: does not fit into V2900/V1280

4444A 10/100/1000 Enet RJ45's

Tom Meier

2000-03-25T11:55:10