L180 Tape Library

Max Configuration:

10 DLT, LTO, SDLT, or 6 9840/9940 Drives

174 Cartridges

Max Native Capacities:

DLT-8000: 216 GB/hr, 7 TB Total

SDLT-320: 576GB/hr, 26.8 TB Total

LTO-1: 540 GB/hr, 17 TB Total

LTO-2: 1.08TB/hr, 33.6 TB Total

9840A: 216 GB/hr, 3.5 TB Total

9840B: 410GB/hr, 3.5 TB Total

9840C: 648GB/hr, 7 TB Total

9940B: 648GB/hr, 35 TB Total

Tape Drive Configurations

Drive Column

with (10) DLT

Tape Drives

Drive Column

with (10) LTO

Tape Drives

Drive Column

with (6) 9840

Tape Drives

Drive Column

with (4) 9840

and (4) LTO

Tape Drives

Configuration Notes:

The tape drives must be all SCSI or all Fibre

If mixing different tape drive technologies,

then ACSLS must be used to partition the library

Drive Column 0

Cartridge Access Port (CAP)

Handles 10 cartridges

Cartridge Expansion (Optional)

Note: If used, increases cartridge

capacity by 100 cartridge slots

Cartridge Capacities

Available Cartridge Capacities:

80 slots

180 slots

Fibre Connectivity

8 Port

Sun FC

Switches

Library

Controller

9840--FC

or

LTO-FC

Tape Drive

9840--FC

or

LTO-FC

Tape Drive

9840--FC

or

LTO-FC

Tape Drive

9840--FC

or

LTO-FC

Tape Drive

9840--FC

or

LTO-FC

Tape Drive

9840--FC

or

LTO-FC

Tape Drive

Configuration Notes

Maximum of three 9840A-FC / 9840B-FC drives per switch zone

Maximum of four hosts per tape drive (switch zone)

Sun L180 Tape Library

Personality Module

10BaseT

Ethernet

Site Plan

2 ft x 2 ft

Tile

100 VAC

Single Phase

15 amps

NEMA 5-15P

(2nd power cord required

if second PDU is used)

L180 Tape Library

28.3" Width

49.3" Depth

65.1" Height

L180

Tape Library

39.6” Maintenance

Space

2” Cooling

Space

8.5 ft

5.9 ft

Sun L180 Tape Library

L180

Jim Miller

2002-06-15T22:07:29