Your Name Here

Your Job Function Here

March 29, 2004

Product Presentation

Volume Servers

B1600 Blades

Chassis with 16 Blade Servers

Administration Tools

V210 Server

2 USIIIi CPU's - 1 GHz

8 GB memory

2 internal 36 GB disks

V240 Server

2 USIIIi CPU's - 1.28 GHz

8 GB memory

4 internal 36 GB disks

V100 Server

1 USII CPU - 650 MHz

4 GB Memory

2 internal disks 40 GB IDE disks

V120 Server

1 USII CPU - 650 MHz

4 GB Memory

2 internal disks 36 GB SCSI disks

V440 Server

4 USIIIi CPU's – 1.28 GHz

16 GB memory

4 internal 36 GB Disks

Volume Servers

V480 Server

4 USIII CPU's – 1.2 GHz

32 GB memory

2 internal 73 GB Disks

280R Server

2 USIII CPU's - 1.2 GHz

8 GB memory

2 internal 36 GB Disks

V250 Server

2 USIIIi CPU's - 1.28 GHz

8 GB memory

8 internal 73 GB Disks

V880 Server

8 USIII CPU's - 1.2 GHz

64 GB memory

12 internal 146 GB disks

Volume Servers
Linux or Solaris x86

V60x Server

2 Intel CPU's - 2.8 or 3.2 GHz

6 GB memory

3 internal 73 GB disks

Solaris x86 or Linux

V65x Server

2 Intel CPU's - 3.2 GHz

12 GB memory

6 internal 73 GB disks

Solaris x86 or Linux

V20z Server

2 AMD Opteron CPU's - 1.6, 1.8 or 2.2 GHz

16 GB memory

2 internal 73 GB disks

Solaris x86 or Linux

Workstations

Sun Ray 150

Sun Ray 100

Sun Blade 150

650 MHz USII CPU

Sun Blade 1500

1 GHz USIIIi CPU

Sun Blade 2500

2x 1.28 GHz USIIIi CPU

Sun Ray 1g

Enterprise Servers

E6900 Server

24 USIV CPU's

192 GB memory

4 Domains

E4900 Server

12 USIV CPU's

96 GB memory

2 Domains

E2900 Server

12 USIV CPU's

96 GB memory

E20K Server

36 USIV CPU's

288 GB memory

9 domains

E25K Server

72 USIV CPU's

576 GB memory

18 domains

Disk Storage

9980

1024 Disks, 147 TB

64 Host interfaces

64 GB cache

9970

128 Disks, 18 TB

48 Host interfaces

32 GB cache

S1

3 146 GB LVD Disks

3310

12 146 GB LVD Disks

3510

12 146 GB FC Disks

2 GB Cache

6320

11 6120 Arrays

Dual 16 port 2 GB Switches

1 Service Processor

45 TB

22 GB Cache

6120 Array

28 146 GB FC Disks

4 TB

2 GB Cache

3310

4 146 GB U320 Disks

D240

DVD

2 73 GB Disks

DDS-4 Tape

Tape Storage

L180 Tape Library

Drives: 10 SDLT320, 10 LTO2

or 6 9840

174 Cartridges

L700 Tape Library

20 SDLT320, 20 LTO2, 12 9840,

or 12 9940 Drives

678 Cartridges

L25 Tape Library

Drives: 2 SDLT320 or 2 LTO

Cartridges: 21 SDLT320 or 25 LTO

L100 Tape Library

Drives: 6 SDLT320 or 6 LTO

Cartridges: 100 SDLT320

or 84 LTO

Tape Drive Comparison

Throughput	Capacity

Type	MB/sec	GB/hr	GB/tape

SDLT320	16	57	160

LTO	15	54	100

LTO2	30	108	200

9840C	30	108	40

9940B	30	108	200

All capacities are native uncompressed

capacities.

L6000 Tape Library

80 9840, or 80 9940B Drives

6000 Cartridges

Can Link 26 L6000's together

L8 Tape Library

1 Drive: SDLT320, LTO

or LTO2

8 Cartridges

Volume Server Details

Sun Rack 900

V880 Server

8 CPU's, 12 Disks

V100 Server

1 CPU, 1 Disk

V480 Server

4 CPU's, 2 Disks

V280 Server

2 CPU's, 2 Disks

V120 Server

1 CPU, 1 Disk

V120

V100

V210 Server

2 CPU's, 2 Disks

V240 Server

2 CPU's, 4 Disks

.The V880 needs a

rack specific mount

kit.

V20z is not

supported in this

cabinet.

Sun 72” Cabinet

V60x Server

2 CPU's, 2 Disks

V65x Server

2 CPU's, 6 Disks

V880

V880 Rack Mount Kit

Sun Rack 900

V480

V210

V280

V240

V60x

V65x

B1600 Blades

16 Blade Servers

B1600

V440

V440 Server

4 CPU's, 4 Disks

V20z

V20z Server

2 CPU's, 2 Disks

Sun Fire Blades

SPARC

I2C

5

DC

Midplane

Switch

System

Controller

10/100/1000 Cat-5 Enet RJ45

LOM Serial Port RJ45

10/100 System MgmtLink RJ45

16

GBE

2

SC-SC

Link

16

Serial

Mgmt

Link

5

I2C

Switch

System

Controller

LOM Serial Port RJ45

10/100 System MgmtLink RJ45

16

GBE

2

SC-SC

Link

16

Serial

Mgmt

Link

5

I2C

PSU

Power

I2C

5

DC

PSU

Power

Sun Fire

B1600

Chassis

Space

for

Blade

Gbe

Gbe

Serial

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Sun Fire B1600

Integrated Switches &System Controller

Redundant Power, 3 RU Chassis

Ships with:

Rack Mount Kit for Sun Rack 900

& Sun 72” Cabinet

Content Load Balancing

B10n

1.5

GHz

AMD

30

GB

Disk

1 GB

B100x

SSL Proxy Blade

B10p

x86

Specialty

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

1.5

GHz

AMD

30

GB

Disk

2 GB

B100x

30

GB

Disk

1 GB

B200x

1 GB

2.0

GHz

Intel

2.0

GHz

Intel

30

GB

Disk

1 GB

B200x

1 GB

2.0

GHz

Intel

2.0

GHz

Intel

30

GB

Disk

512

MB

B100s

650

MHz

USII

30

GB

Disk

1

GB

B100s

650

MHz

USII

30

GB

Disk

2

GB

B100s

650

MHz

USII

V100 Server

V100

1 USII CPU - 650 MHz

1 GB memory (4 GB Max)

2 internal disks (IDE) - 40 GB each

CD-ROM

1 Rack Unit High (1.75 in.)

Included Rack Mount Kit fits:

Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

V100

USB

Serial

Power

CDROM

40 GB disk

Space for Memory

10/100 Enet

Space for Memory

10/100 Enet

Serial

512 MB memory

512 MB memory

Space

for disk

40 GB disk

650 MHz

USII

System Config Card

V120 Server

V120

1 USII CPU - 650 MHz

1 GB memory (4 GB max)

36 GB internal SCSI disk (2 max)

Slot for CD-ROM or DVD

33 MHz PCI slot

1 Rack Unit High (1.75 in.)

Included Rack Mount Kit fits

Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

V120

USB

Power

650 MHz

USII

Space for Memory

Space for Memory

10/100 Enet RJ45

Serial DB9

Space for

CDROM

or DVD

UltraSCSI HD68

33 MHz PCI Slot

System Config Card

10/100 Enet RJ45

Serial DB9

Space

for Disk

Space for Memory

Space for Memory

Space

for Disk

36 GB

Disk

36 GB

Disk

256 MB memory

256 MB memory

V210 Server

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

V210 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

ALOM

Space for Sun Crypto

Accelerator 500

Space

for

CPU

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Space

for Disk

Space

for Disk

V210 Server

Capacity:

2 USIIIi CPU's - 1.06 GHz each

8 GB memory

2 internal 36 or 73 GB LVD disks

1 PCI Cards - 66 MHz

4 10/100/1000Base -T Ethernet Ports

DVD Drive Option

Sun Crypto Accelerator Card Option

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Single Power Supply.

Single Power Cord

1 Rack Unit high

Ships with:

Rack Mounting with cable management

fits Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

System Key

RJ-45 to DB-9 Adapter

RJ-45 to DB-25 Adapter

Cat5 RJ-45 cable

2 CPU, 2 GB memory, 2x 36 GB disk, base configuration

1 CPU, 512 MB memory, 1x 36 GB disk, base configuration

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

V210 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

ALOM

Space for Sun Crypto

Accelerator 500

Space

for

CPU

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Space

for Disk

Space

for Disk

36 GB

Disk

512 MB

1.06

GHz

USIIIi

36 GB

Disk

36 GB

Disk

1.06

GHz

USIIIi

1.06

GHz

USIIIi

1 GB

1 GB

Disk Options

36 GB

Disk

73 GB

Disk

DVD

DVD Option

Memory Options

1 GB

2 GB

512 MB

V240 Server

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

System Config Card

33 MHz PCI Slot

33 MHz PCI Slot

Power Supply

Power

V240 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

ALOM

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space for Sun Crypto

Accelerator 500

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

System Config Card

33 MHz PCI Slot

33 MHz PCI Slot

Power Supply

Power

V240 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

ALOM

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space for Sun Crypto

Accelerator 500

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

V240 Server

Capacity:

2 USIIIi CPU's - 1.06 or 1.28 GHz each

8 GB memory

4 internal 36 or 73 GB LVD disks

3 PCI Cards - 1x 66 MHz, 2x 33 MHz

4 10/100/1000Base -T Ethernet Ports

DVD Drive Option

Sun Crypto Accelerator Card Option

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Redundant Power Supplies.

2 Power Cords

2 Rack Units high

Ships with:

Rack Mounting with cable management

fits Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

System Key

RJ-45 to DB-9 Adapter

RJ-45 to DB-25 Adapter

Cat5 RJ-45 cable

2 CPU, 8 GB memory, 2x 36 GB disk, base configuration

1 CPU, 512 MB memory, 1x 36 GB disk, base configuration

Disk Options

36 GB

Disk

73 GB

Disk

DVD

DVD Option

Memory Options

1 GB

2 GB

1.06

GHz

USIIIi

512 MB

36 GB

Disk

1.28

GHz

USIIIi

1.28

GHz

USIIIi

2 GB

2 GB

2 GB

2 GB

36 GB

Disk

36 GB

Disk

512 MB

V250 Server

V250 Server

Capacity:

2 USIIIi CPU's - 1.06 or 1.28 GHz each

8 GB memory (4 GB per CPU)

8 internal 36 or 73 GB Ultra160 SCSI disks

6 PCI Cards - 3x 66/33 MHz, 3x 33 MHz

1 10/100/1000Base -T Ethernet Port

DVD Drive

Optional DDS4- DAT tape drive

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Redundant Power Supplies.

2 Power Cords

1 CPU, 512 MB memory, 1x 36 GB disk, base configuration

2 CPU's, 8 GB memory, 2x 73 GB disk, base configuration

Disk Options

DDS-4 Tape

Tape Option

Memory Options

1 GB

2 GB

36 GB Disk

73 GB Disk

Space for

DAT tape

Power

2x USB 1.0

LVD SCSI VHDCI

Serial Port RJ45

10/100/1000 Cat-5 Enet RJ45

10/100 Enet RJ45

System Config Card

Serial Port DB9

ALOM

V250 Server

Parallel Port DB25

2x USB 1.0

DVD drive

Power Supply

Power

Power Supply

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space

for

CPU

Space

for

CPU

Space for

Disk

1.06

GHz

USIIIi

512 MB

36 GB Disk

Space for

DAT tape

Power

2x USB 1.0

LVD SCSI VHDCI

Serial Port RJ45

10/100/1000 Cat-5 Enet RJ45

10/100 Enet RJ45

System Config Card

Serial Port DB9

ALOM

V250 Server

Parallel Port DB25

2x USB 1.0

DVD drive

Power Supply

Power

Power Supply

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space

for

CPU

Space

for

CPU

Space for

Disk

1.28

GHz

USIIIi

1.28

GHz

USIIIi

2 GB

2 GB

2 GB

2 GB

73 GB Disk

73 GB Disk

512 MB

280R Server

280R Server

2 USIII CPU's - 1.2 GHz

4 GB memory (8 GB max)

2 internal 36 disks

4 PCI Cards - 1x 66 MHz, 3x 33 MHz

DVD Drive

N+1 Power & Fans.

Dual Power Cords

4 Rack Units (7 in.) high

Included Rack Mount Kit fits

Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

66 MHz PCI Slot

33 MHz PCI Slot

Space for Memory

DVD drive

Serial A / B

56k modem

Remote System

Control

10 Ethernet

Power Supply

Power

Power Supply

Power

USB

280R Server

UltraSCSI HD68

Space for

CPU

10/100 Enet RJ45

Serial A/B DB27

33 MHz PCI Slot

33 MHz PCI Slot

Space

for Disk

Space

for Disk

Space for

CPU

Space for Memory

1.2 GHz

USIII

1.2 GHz

USIII

2 GB memory

2 GB memory

36 GB

Disk

36 GB

Disk

V440 Server

DVD drive

Power Supply

Power

V440 Server

Ultra320 SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

Power Supply

Power

ALOM

USB

USB

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

#0

#4

#3

#2

#1

#5

2 CPU's, 4 GB memory, 4 x 36 GB disk, base configuration

4 CPU's, 16 GB memory, 4 x 36 GB disk, base configuration

V440 Server

Capacity:

4 USIIIi CPU's - 1.062 or 1.28 GHz each

16 GB memory (4 GB per CPU)

4 internal 36 or 73 GB Ultra320 SCSI disks

6 PCI Cards - 3x 66/33 MHz, 3x 33 MHz

2 10/100/1000Base -T Ethernet Ports

DVD Drive

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Redundant Power Supplies.

2 Power Cords

4 Rack Units high

Ships with:

Rack Mounting with cable management

fits Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

System Key

RJ-45 to DB-9 Adapter

RJ-45 to DB-25 Adapter

Cat5 RJ-45 cable

Disk Options

36 GB

Disk

73 GB

Disk

36 GB

Disk

36 GB

Disk

36 GB

Disk

36 GB

Disk

1 GB

1.06

GHz

USIIIi

1 GB

1 GB

1.06

GHz

USIIIi

1 GB

DVD drive

Power Supply

Power

V440 Server

Ultra320 SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

Power Supply

Power

ALOM

USB

USB

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

#0

#4

#3

#2

#1

#5

36 GB

Disk

36 GB

Disk

36 GB

Disk

36 GB

Disk

2 GB

1.28

GHz

USIIIi

2 GB

2 GB

1.28

GHz

USIIIi

2 GB

2 GB

1.28

GHz

USIIIi

2 GB

2 GB

1.28

GHz

USIIIi

2 GB

V480 Server

V480 Server

4 USIII CPU's – 1.2 GHz

32 GB memory

2 internal 73 GB FCAL disks

DVD

6 PCI Cards - 2x 66 MHz, 4x 33 MHz

2x 10/100/1000 Cat-5 Ethernet

N+1 Power & Fans.

Dual Power Cords

5 Rack Units (8.75 in.) high

Included Rack Mount Kit fits

Sun 900 Rack & Sun 72” Cabinet

V480 Server

66 MHz PCI Slot

33 MHz PCI Slot

DVD

Serial A / B

56k modem

Remote System

Control

Ethernet 10

Space

for

CPU / Memory

Board

Power Supply

USB

Serial RJ45

Power

Power Supply

Power

Space

for

CPU / Memory

Board

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Space

for Disk

Space

for Disk

36 GB

Disk

36 GB

Disk

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

V880 Server

V880 Server

8 USIII CPU's - 1.2 GHz

16 GB memory (64 GB max)

6 internal 73 GB FCAL disks (12 max)

DVD

9 PCI Cards - 2x 66 MHz, 7x 33 MHz

10/100 Enet

Fiber 1000 Enet

N+1 Power & Fans.

3 Power Cords

17 Rack Units high

X9638A Sun 900 Rack Mount Kit

X9628A Sun 72” Cabinet Mount Kit

X6756A

Second Backplane

with 6x 73 GB Disks

Second Backplane

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

73

GB

73

GB

73

GB

73

GB

73

GB

73

GB

Second Backplane

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

146

GB

146

GB

146

GB

146

GB

146

GB

146

GB

X6858A

Second Backplane

with 6x 146 GB Disks

Serial A / B

56k modem

Remote System

Console

66 MHz PCI Slot

66 MHz PCI Slot

Space for Disk Backplane

Ethernet 10

33 MHz PCI Slot

DVD

Space for Tape

Space

for

CPU / Memory

Board

Internal SCSI

Space

for

CPU / Memory

Board

Space for Tape

73

GB

73

GB

73

GB

73

GB

73

GB

73

GB

Power Supply

Power

USB

Serial

Power Supply

Power

Power Supply

Power

Space

for

CPU / Memory

Board

Space

for

CPU / Memory

Board

10/100 Enet RJ45

Gb Enet SC

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Serial

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

Internal Cable Option

X6755A

6727A Dual Gb FC

SC

SC

V20z Server

V20z Server

Capacity:

1 or 2 AMD Opteron CPU's - 1.6, 1.8 or 2.2 GHz

1 - 16 GB memory

1-2 internal U320 SCSI (36/73) disk drives

CD + Floppy Drive

2 PCI-X Card Slots - 133/66 MHz

1 Full-Size 133/66 MHz , 1 Low Profile 66 MHz

2 10/100/1000 BaseT Ethernet Ports

1 USB port

PS/2 keyboard / mouse support

IPMI System Processor

1 power cord

1 Rack Unit high

X9274A Rack Mount Kit for Sun Rack 900

Not Supported in 72” Cabinet

Ships with:

Linux Resource CD (drivers, IPMI utils, etc.)

1x 1.6 MHz CPU, 1 GB memory, 1x 36 GB disk configuration

2x 2.2 GHz CPU's, 4 GB memory, 2x 36 GB disk configuration

DVD + Floppy

Flex Bay Options

Disk Options

9265A U320 SCSI

VHDCI

VHDCI

Memory

1 GB

2 GB

9271A 1000/100/10 Enet

RJ45

9272A 1000/100/10 Enet

RJ45

RJ45

9273A Quad 1000/100 Enet RJ45's

4 GB

133 MHz Only

Full Size Only

9279A 2 Gb FC-AL

LC

PCI-X Cards

Low Profile (also fits Full Size Slot)

36 GB

Disk

USB

V20z Server

Serial Port DB9

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

Keyboard PS/2

Full size 133/66 MHz PCI-X Slot

Video DB15

CD + Floppy

Flex Bay

Low Profile 66 MHz PCI-X slot

Mouse PS/2

10/100 Enet RJ45

10/100 Enet RJ45

IPMI

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

1 GB

36 GB

Disk

1.6 GHz

Opteron

CPU

USB

V20z Server

Serial Port DB9

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

Keyboard PS/2

Full size 133/66 MHz PCI-X Slot

Video DB15

CD + Floppy

Flex Bay

Low Profile 66 MHz PCI-X slot

Mouse PS/2

10/100 Enet RJ45

10/100 Enet RJ45

IPMI

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

36 GB

Disk

2.2 GHz

Opteron

CPU

2.2 GHz

Opteron

CPU

2 GB

2 GB

36 GB

Disk

73 GB

Disk

V60x Server

V60x Server

Capacity:

1 or 2 Intel Xeon 2.8 or 3.2 GHz CPU's

512MB- 6 GB memory

1-3 internal U-320 LVD (36/73) disk drives

CD + Floppy Drive

2 PCI-X Card Slots - 100/66/33 MHz

1 Full-Size, 1 Low-Profile PCI

2 10/100/1000 BaseT Ethernet Ports

3 USB ports

PS/2 keyboard / mouse support

Graphics support up to 1600 x 1200

IPMI for remote management

1 power cord

1 Rack Unit high

X5030A Rack Mount Kit for Sun Rack 900 & 72” Cabinet

X5137A Serial & RJ45 dongle kit

Ships with:

Linux Resource CD (drivers, IPMI utils, etc.)

PS/2 "Y" splitter

1x 2.8 GHz CPU, 512 MB memory, 1x 36 GB disk configuration

2x 3.2 GHz CPU's, 1 GB memory, 1x 36 GB disk configuration

DVD + Floppy

Flex Bay Options

Disk Options

PCI Card Options

5132A RAID Controller

5133A 1 Gb FC

SC

Memory Options

256 MB memory

256 MB memory

512 MB memory

512 MB memory

1 GB memory

1 GB memory

USB

V60x Server

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

DB15 Video

Keyboard & Mouse

100/66/33 MHz PCI-X Slot

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

CD + Floppy

Flex Bay

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

Low Profile PCI-X Slot

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

3.2 GHz

Xeon

CPU

512 MB memory

512 MB memory

3.2 GHz

Xeon

CPU

36 GB

Disk

USB

V60x Server

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

DB15 Video

Keyboard & Mouse

100/66/33 MHz PCI-X Slot

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

CD + Floppy

Flex Bay

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

Low Profile PCI-X Slot

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

36 GB

Disk

256 MB memory

256 MB memory

2.8 GHz

Xeon

CPU

36 GB

Disk

73 GB

Disk

36 GB

Disk

73 GB

Disk

V65x Server

1x 2.8 GHz CPU, 512 GB memory, 1x 36 GB disk configuration

V65x Server

Capacity:

1 or 2 Intel Xeon CPU's, 2.8 GHz or 3.2 GHz

512MB- 12 GB memory

1-6 internal U-320 LVD (36/73) disk drives

CD + Floppy Drive

6 PCI-X Cards - 100/66/33 MHz

3 Full-size PCI slots, 3 Low-profile slots

2 10/100/1000 BaseT Ethernet Ports

3 USB ports

PS/2 keyboard / mouse support

Graphics support up to 1600 x 1200

IPMI for remote management

Redundant Power Supply Option.

1 Power Cords per Power Supply

2 Rack Units high

X5030A Rack Mount Kit for Sun Rack 900 & 72” Cabinet

X5137A Serial & RJ45 dongle kit

Ships with:

Linux Resource CD (drivers, IPMI utils, etc.)

PS/2 "Y" splitter

DVD + Floppy

36 GB

Disk

73 GB

Disk

2x 3.2 GHz CPU, 1 GB memory, 1x 36 GB disk configuration

Power

2nd Power Supply

5132A RAID Controller

Flex Bay Options

Disk Options

PCI Card Options

Memory Options

256 MB memory

256 MB memory

512 MB memory

512 MB memory

1 GB memory

1 GB memory

2 GB memory

2 GB memory

Redundant Power Option

5133A 1 Gb FC

SC

USB

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Space for Power Supply

DB15 Video

Keyboard & Mouse

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

Power Supply

Power

V65x Server

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

Low Profile PCI-X Slot

Flex Bay

CD + Floppy

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

Low Profile PCI-X Slot

Low Profile PCI-X Slot

3.2 GHz

Xeon

CPU

512 MB memory

512 MB memory

3.2 GHz

Xeon

CPU

36 GB

Disk

USB

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Space for Power Supply

DB15 Video

Keyboard & Mouse

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

Power Supply

Power

V65x Server

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

Low Profile PCI-X Slot

Flex Bay

CD + Floppy

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

Low Profile PCI-X Slot

Low Profile PCI-X Slot

36 GB

Disk

256 MB memory

256 MB memory

2.8 GHz

Xeon

CPU

Sun Blade 150 Workstation

Sun Blade 150

USB

Serial

Parallel

Power

512 MB memory

DVD-ROM

Floppy Drive

Sun Blade 150

1 CPU -550 or 650 MHz

512 MB memory (2 GB max)

80 GB internal disk (2 max)

DVD-ROM (CD-RW Optional)

Floppy Drive

3 PCI Slots - 33 MHz

Space

for disk

80 GB disk

Space for Memory

10/100 Enet RJ45

33 MHz PCI

33 MHz PCI

33 MHz PCI

Space for Memory

PGX64 HD15

Space for Memory

650 MHz

USII CPU

Sun Blade 1500 Workstation

Sun Blade 1500

Power

DVD

Sun Blade 1500

1 GHz CPU

512 MB memory (4 GB max)

80 GB ATA-100 internal disk (2 max)

DVD ROM Drive

Smart Card Reader

4 USB 1.1, 3 USB 2.0 and 2 IEEE 1394 ports

Sun XVR-100 Graphics Accelerator

Optional Sun XVR-500

2 serial, 1 parallel ports

Gigabit Ethernet on-board

5 PCI Slots

- 1 x 64-bit 66 MHz

- 2 x 64-bit 33 MHz

- 2 x 32-bit 33 MHz

Smart Card Reader

Headphones / Mic

2x USB 1.1

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

64 bit 33 MHz PCI Slot

64 bit 33 MHz PCI Slot

Parallel Port DB25

2x USB 1.1

64 bit 33 MHz PCI Slot

64 bit 66 MHz PCI Slot

Space for

Disk

Space for

Disk

80 GB

ATA Disk

Space

for

CPU

1.06

GHz

USIIIi

USB/IEEE

3 USB 2.1 Ports

2 IEEE 1394 ports

Audio Serial DB9 / Headphones/Mic

512 MB

XVR-100 Graphics DB15/DVI-I/DIN7

64 bit 33 MHz PCI Slot

1.06 GHz CPU, 512 MB memory, 80 GB disk, XVR 100

Sun Blade 2500 Workstation

Sun Blade 2500 Workstation

Capacity:

2 CPU's - 1.28 GHz each

8 GB memory (4 GB per CPU)

2 internal 36 GB Ultra160 SCSI disks

6 PCI Cards - 3x 66/33 MHz, 3x 33 MHz

1 10/100/1000Base -T Ethernet Port

DVD Drive

Smart Card Reader

1 CPU, 1 GB memory, 36 GB disk, XVR 100

Second Bay

2x USB 1.1

LVD SCSI VHDCI

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

64 bit 33 MHz PCI Slot

64 bit 33 MHz PCI Slot

Power

Sun Blade 2500

Parallel Port DB25

2x USB 1.1

64 bit 33 MHz PCI Slot

64 bit 66 MHz PCI Slot

Space for

Disk

Space for

Disk

36 GB

LVD Disk

DVD drive

Space

for

CPU

1.28

GHz

USIIIi

USB/IEEE

3 USB 2.x Ports

2 IEEE 1394 ports

Audio Serial DB9 / Headphones/Mic

Not Usable

64 bit 66 MHz PCI Slot

64 bit 66 MHz PCI Slot

XVR-100 Graphics DB15/DVI-I/DIN7

2 CPU's, 2 GB memory, 36 GB disk, XVR 500

XVR-500 Graphics DB15/DIN7

Smart Card Reader

Factory

Install

Only

Not Usable

1 GB

Second Bay

2x USB 1.1

LVD SCSI VHDCI

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

64 bit 33 MHz PCI Slot

64 bit 33 MHz PCI Slot

Power

Sun Blade 2500

Parallel Port DB25

2x USB 1.1

64 bit 33 MHz PCI Slot

64 bit 66 MHz PCI Slot

Space for

Disk

Space for

Disk

36 GB

LVD Disk

DVD drive

USB/IEEE

3 USB 2.x Ports

2 IEEE 1394 ports

Audio Serial DB9 / Headphones/Mic

64 bit 66 MHz PCI Slot

64 bit 66 MHz PCI Slot

XVR-100 Graphics DB15/DVI-I/DIN7

Smart Card Reader

Space

for

CPU

1.28

GHz

USIIIi

Space

for

CPU

1.28

GHz

USIIIi

2 GB

Sun Rays

Sun Ray 1g

ATI Radeon 7000 Graphics DVI/I

Power

10/100 Enet RJ45

Processor

2x USB

2x USB

Stereo Audio Out

Stereo Audio In

Smart Card Reader

Headphones

Microphone

Sun Ray 100

Integrated 17” CRT

Sun Ray 150

Integrated 15” LCD

Sun Ray 1g with 24” LCD Monitor

Smart Card Reader conforming to ISO-7816-1

ATI Radeon 7000 Graphics, 24-bit graphics,

Up to 1920x1200 @ 75 Hz, DVI/I Connector

Supports Sun’s 24” LCD Flat Panel monitor and

via included HD15 adapter :

Sun's 17-in. and 21-in Monitors

Sun’s 18-in. LCD flat panel

Standard VGA compatible monitors

10BASE-T/100BASE-T Ethernet (RJ-45)

Four standard Universal Serial Bus (USB) Type A ports, powered

Four 16-bit stereo audio ports using standard 0.125-inch (3.5-mm) jacks

Front - headphone(out) and microphone(in)

Rear - line-in and line-out

Supports Type 6 USB keyboard and Type 6 USB mouse

Ships with

Stand

DVI/I to HD15 Adapter

Sun Monitors

24.1 inch AM TFT LCD

1920 x 1200 Max Resolution

Ships with:

13W3/13W3 Video Cable

DVI-D/DVI-D Video Cable

S-Video Cable

C-Video Cable

USB Cable

17 inch Color CRT

1280 x 1024 Max Resolution

Attached HD15 video Cable

22 inch FD Trinitron CRT

1600 x 1200Max Resolution

Attached 13W3 Video Cable

Separate HD15 Connector

19 inch LCD

1280 x 1024 Max Resolution

DVI-I Video Connector

HD15 Connector

DVI-D to DVI-D cable

HD15 to HD15 cable

E2900 Server

E2900 Server

12 USIV CPU's - 1.2 GHz (1.05 GHz available)

48 GB memory (96 GB max)

2 internal 73 GB LVD SCSI disks

DVD

DDS-4 Tape Option

6 PCI Cards - 1x 66 MHz, 5x 33 MHz

2x 10/100/1000 Cat-5 Ethernet

2N Power & Fans.

4 Power Cords

12 Rack Units high

Included Rack Mount Kit works with

Sun 900 Rack & Sun 72” Cabinet

E2900 Server

LVD SCSI VHDCI

DVD

Space

for Disk

PCI 0 – 33 MHz Slot

Standby System Controller

Version 2

Ethernet 10/100 RJ45

Space

for

CPU

Memory

Board

L2 Address Repeater Switch

L2 Address Repeater Switch

Alarms Port DB15

Space for

DDS-4 Tape

PCI 1 – 33 MHz Slot

PCI 2 – 33 MHz Slot

PCI 3 – 33 MHz Slot

PCI 4 – 33 MHz Slot

PCI 5 – 66 MHz Slot

System Config Card

10/100/1000 Cat-5 Enet RJ45

Power Supply 0

Source

B

Serial RJ45

Power Supply 1

Power Supply 2

Power Supply 3

SCSI

Source

A

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Memory

Board

Space

for

CPU

Memory

Board

Space

for Disk

CPU / Memory

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

CPU / Memory

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

CPU / Memory

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

1.2 GHz

USIV

2 GB

2 GB

73 GB

LVD Disk

73 GB

LVD Disk

E4900 Server

2 D240 Media Trays

Each with: DVD

2 x 73 GB disks

DDS-4 Tape Drive

E4900 Server

12 USIV CPU's - 1.2 GHz (1.05 GHz available)

48 GB Memory (96 GB max)

Domain Configuration

Label	Function	Segment	CPU's	Memory

A	Production	0	4	8 GB

B	(not available)

C*	Staging	1	8	16 GB

D*	(not available)

* Segmenting the system enables use of these

Domains

NOTE: Each Domain requires at least one

CPU / Memory Board and one I/O Assembly.

F4800

D240

D240

Fan Tray

L2 Address Repeater Switch

A

A

C

C

Fan Tray

Fan Tray

Power Supply

Power Supply

Power Supply

L2 Address Repeater Switch

A

C

C

66

33

33

33

66

33

33

33

Top I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

Bottom I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Serial A/B DB25

100/10 Ethernet RJ45

System Controller

Version 2

Serial A/B DB25

100/10 Ethernet RJ45

System Controller

Version 2

Space for

Uniboard

Space for

Uniboard

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Space for

Uniboard

Space for

Uniboard

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

Space for

Uniboard

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

E6900 Server

Domain Configuration

Label	Function	Segment	CPU's	Memory

A	Production	0	12	48 GB

B	(available)	0

C*	Staging	1	12	48 GB

D*	(available)	1

* Segmenting the system enables use of these

Domains

NOTE: Each Domain requires at least one

CPU / Memory Board and one I/O Assembly.

2 D240 Media Trays

Each with: DVD

2 x 73 GB disks

DDS-4 Tape Drive

E6900 Server

24 USIV CPU's - 1.2 GHz

(1.05 GHz available)

96 GB Memory (192 GB max)

F6900

D240

D240

PS

L2 Address Repeater Switch

L2 Address Repeater Switch

L2 Address Repeater Switch

L2 Address Repeater Switch

PS

PS

PS

PS

PS

A

A

A

C

A

A

C

A

C

C

C

C

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Left I/O Assy - PCI

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Bottom Right I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Right I/O Assy - PCI

66

33

33

33

66

33

33

33

Bottom Left I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

Space for

Uniboard

DB25 Serial A/B

RJ45 100/10 Ethernet

System Controller

Version 2

DB25 Serial A/B

RJ45 100/10 Ethernet

System Controller

Version 2

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

Domain Example

Domain A: Production

A

A

A

A

66

33

33

33

66

33

33

33

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Bottom Right I/O Assy - PCI

66 MHz PCI Slot

33 MHz PCI Slot

66

33

33

33

66

33

33

33

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

Top Right I/O Assy - PCI

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

6120 2x2

4 TB Disk, 2 GB cache

A

B

6120 Disk Array

Space for RAID Controller

RJ45 Serial

RJ45 Enet

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146

H/W RAID Controller

with 1 GB Cache

LC FC

A

B

Space for RAID Controller

RJ45 Serial

RJ45 Enet

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146

H/W RAID Controller

with 1 GB Cache

LC FC

146

146

LC-LC fiber

5 meters

incl w/ 6120

LC-LC fiber

5 meters

incl w/ 6120

SG-PCI1FC-QF2 2Gb FC

LC

SG-PCI1FC-QF2 2Gb FC

LC

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

73 GB

73 GB

73 GB

DVD

HD68

HD68

HD68

HD68

D240

VHDCI-HD68

4 meters

X3830A

X3830A

E20K/E25K Server Details

Boot Disks

Mirrored S1's

Sun Rack 900

Sun Fire E25K Server

72 USIV CPU's

576 GB memory

18 domains

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

S1

E25K Server

Domain	Use	CPUs	Memory	Usable Disk

A	Production	12	48 GB	290 GB*

B	Production	8	32 GB	608 GB*

C	Production	8	32 GB	524 GB*

D	Production	8	32 GB	276 GB*

E	Production	8	32 GB	55 GB*

*has mirror of same size for backup

E25K Back

Domain	Use	CPUs	Memory	Usable Disk

F	Test	4	16 GB	276 GB

G	Dev	4	16 GB	220 GB

H	B Test & Dev	4	16 GB	608 GB

I	App Rel Testing	16	48 GB	939 GB

Available: 2867 GB

Total	72	288 GB	6.6 TB

E25K Front

8

7

6

5

4

3

2

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

1

0

17

16

15

14

13

12

11

10

9

Sys Control #1

Sys Control #2

System

Controller

Board

Serial DB9

Ethernet RJ45

CPU

Card

Ethernet RJ45

System

Controller

Board

RJ45 Ethernet

DB9 Serial

CPU

Card

RJ45 Ethernet

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

Domain A

Domain B

Domain C

Domain D

Domain E

Domain F

Domain G

Domain H

Domain I

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

E20K Server

E20K Back

Domain	Use	CPUs	Memory	Usable Disk

A	Production	12	48 GB	290 GB*

B	Production	8	32 GB	608 GB*

C	Production	8	32 GB	524 GB*

D	Production	8	32 GB	276 GB*

Total	36	144 GB	1.8 TB

*has mirror of same size for backup

8

7

6

5

4

3

2

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

Space

for

System

Controller

Board

Space

for

S C

Per'l

Board

S C

Peri'l

Board

18 GB

Disk

18 GB

Disk

DVD

Tape

1

0

17

16

15

14

13

12

11

10

9

Sys Control #1

Sys Control #2

System

Controller

Board

Serial DB9

Ethernet RJ45

CPU

Card

Ethernet RJ45

System

Controller

Board

RJ45 Ethernet

DB9 Serial

CPU

Card

RJ45 Ethernet

Slots 9-17 are disabled.

Upgrade is available to enable.

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

Uniboard

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

2 GB

2 GB

1.2

GHz

USIV

E20K Front

Domain A

Domain B

Domain C

Domain D

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

hsPCI+

2222A

3150A

SG-PCI1FC-QF2

E20K/E25K Domain Example

0

S1: Boot Disks

36

36

36

HD68

HD68

36

36

36

HD68

HD68

VHDCI-HD68

10 meters

VHDCI-HD68

10 meters

X3831A

X3831A

S1: Boot Disks Mirror

16

GB

LC A

StorEdge 9980

16

GB

DKA

#4

DKA

#2

DKA

#1

DKA

#0

Disk Adapter Boards

Cache Memory

3 GB

Shared Memory

256

73 GB

Disks

(8 spares)

256

73 GB

Disks

(8 Spares)

Space

for

Disk

Frame

CHA

#1

CHA

#2

A LC

Space

for

Disk

Frame

LC B

LC C

LC D

LC E

LC F

LC G

LC H

LC J

LC K

LC L

LC M

B LC

C LC

D LC

E LC

F LC

G LC

H LC

J LC

K LC

L LC

M LC

X9734A

LC-LC fibre

15 meters

X9734A

LC-LC fibre

15 meters

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

66 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66

66

33

66

66 MHz PCI Slot

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

SG-PCI1FC-QF2 2Gb FC

LC

1150A 1000/100/10 Enet

RJ45

1

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

66 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66

66

33

66

66 MHz PCI Slot

2222A

10/100 Enet Dual RJ-45's

LVD SCSI Dual VHDCI's

SG-PCI1FC-QF2 2Gb FC

LC

1150A 1000/100/10 Enet

RJ45

2

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

66 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66

66

33

66

66 MHz PCI Slot

E4900/E6900/E20K/E25K
CPU Board Options

US IV

1.05 GHz

USIV

1.2 GHz

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.2 GHz

USIV

1.2 GHz

USIV

1.2 GHz

USIV

1.05

GHz

USIV

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

2 GB

Uniboard

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

4 GB

Uniboard

1.05

GHz

USIV

1.05

GHz

USIV

1.05

GHz

USIV

PCI Card Options

SCSI Cables

X979A

X973A

SC-SC fibre

2 meters

X978A

HD68 - HD68

SC - SC Fibre

X9715A

VHDCI - HD68

VHDCI - VHDCI

Fibre Cables

SC - LC Fibre

LC / LC Fibre

X1138A

VHDCI-VHDCI

2 meters

X3830B

VHDCI-VHDCI

4 meters

X3831B

VHDCI-VHDCI

10 meters

X1136A

VHDCI-VHDCI

0.8 meter

X3810A

X1132A

VHDCI-HD68

0.8 meter

X1134A

HD68-HD68

0.8 meter

X1139A

HD68-HD68

2 meters

HD68-HD68

4 meters

HD68-HD68

12 meters

X3832A

VHDCI-HD68

2 meters

X3830A

VHDCI-HD68

4 meters

X3831A

VHDCI-HD68

10 meters

SC-SC fibre

5 meters

SC-SC fibre

15 meters

X9722A

SC-LC fibre

2 meters

X9721A

SC-LC fibre

0.4 meter

X9723A

SC-LC fibre

5 meters

X9724A

SC-LC fibre

15 meters

X9735A

SC-LC fibre

25 meters

X9737A

SC-LC fibre

50 meters

X9732A

LC-LC fibre

2 meters

X9733A

LC-LC fibre

5 meters

X9734A

LC-LC fibre

15 meters

X9736A

LC-LC fibre

25 meters

X9738A

LC-LC fibre

50 meters

X1137A

VHDCI-VHDCI

1.2 meters

1034A Quad 100 Enet RJ45's

66/33 MHz PCI Cards

33 MHz PCI Cards

PCI Cards

1155A High Speed Serial 2.0

1071A HIPPI/P 1.1

2156A Serial Async 3.0

1151A Gb Enet

MMF

1150A 1000/100/10 Enet

RJ45

6799A Gb FC

SC

6727A Dual Gb FC

SC

SC

SG-XPCI1FC-QF2 2Gb FC

LC

SG-XPCI2FC-QF2 2Gb FC

LC

LC

6758A Dual LVD SCSI

VHDCI

VHDCI

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

6540A UltraSCSI

VHDCI

VHDCI

6541A UltraSCSI Diff

VHDCI

VHDCI

1157A ATM 155 4.0

MMF

X9739A

SC-SC fibre

100 meters

Was 6767A

Was 6768A

SG-XPCI1FC-JF2 JNI 2Gb

LC

Last Order Data: 4/16/04

Last Order Data: 4/16/04

3151A Gb Enet

MMF

3150A 1000/100/10 Enet

RJ45

SG-XPCI2FC-JF2 JNI 2Gb

LC

LC

1074A SCI cluster

Last Order Data: 6/09/04

Last Order Data: 8/24/04

2222A

10/100 Enet Dual RJ45's

LVD SCSI Dual VHDCI's

Full Length: does not fit into V2900/V1280

4444A 10/100/1000 Enet RJ45's

Site Plan

2 ft x 2 ft

Tile

72" Cabinet

Power cords are

NEMA #L6-30P

200/240 VAC

Single Phase

24 amps each

72" Cabinet

24" Width

37" Depth

73.7" Height

Clearances:

48" Front

36" Back

Sun Rack 900

Power cords are

NEMA L6-20P

200/240 VAC

Single Phase

16 amps each

Sun Rack 900

23.5" Width

35.4" Depth

74" Height

Clearances:

48" Front

36" Back

Power Distribution Sys:

12 outlets per external

power cord

20 internal cords included

24 outlets

24 outlets

9 outlets

9 outlets

11 connects:

7 reg cords

2 split cords

11 connects:

7 reg cords

2 split cords

Optional Front Door

Optional Front Door

Sun Fire 15K

33.25" Width

65" Depth

75" Height

Clearances:

36" Front

36" Back

E25K

Power cords are

NEMA #L6-30P

200/240 VAC

Single Phase

24 amps each

E6900

Power cords are

NEMA #L6-30P

200/240 VAC

Single Phase

30 amps per RTU

E4900

Power cords are

NEMA #L6-30P

200/240 VAC

Single Phase

30 amps per RTU

Sun Fire

Cabinet

24" Width

37" Depth

75" Height

Clearances:

48" Front

36" Back

R

T

S

R

T

S

RTU

Space

for

RTU

R

T

S

R

T

S

RTU

R

T

S

R

T

S

RTU

F6800

Cabinet

24" Width

57" Depth

75" Height

Clearances:

48" Front

36" Back

Disk Array Details

S1

D240

3510

3310

Sun Rack 900

6120

6120

6320

SE9970

SE9980

S1

S1 Disk Array

2 or 3 36, 73, or 146 GB LVD SCSI disks

Will also operate as SCSI-2

1 Rack Unit

Rack Mount Kits:

X6919A: Rack Mount Kit for Sun 900 Rack & Sun 72” Cab

X6920A: Sun Fire Cabinet Rack Mount Kit

Ships with:

146 10k

Disk Options

73 10k

36 10k

146 10k

73 10k

36 10k

146 10k

73 10k

36 10k

Incl w/ S1

HD68-HD68

2 meters

VHDCI-HD68

2 meters

Incl w/ S1

HD68

HD68

S1

36 10k

36 10k

36 10k

VHDCI-HD68

2 meters

Incl w/ S1

D240

D240 Media Tray

DVD

2 x 73 GB disks

DDS-4 Tape Drive

-or-

DVD

3 x 73 GB disks -or-

-or-

4 x 73 GB disks

Features:

N+1 Power & Fans

Hot Swappable Power & Fans

Dual power cords

Dual or Single Ultra SCSI connections

2 Rack Units (3.5 in.) high

Rack Mount Kits:

Included: Sun 72” Cab & Sun Fire Cab

X6839A: Sun Rack 900 Mount Kit

73 GB Disk

HD68 SCSI

73 GB Disk

DDS-4 Tape Drive

DVD

In

Out

In

Out

HD68 SCSI

HD68 SCSI

HD68 SCSI

73 GB

73 GB

Tape

DVD

HD68

HD68

HD68

HD68

D240

VHDCI-HD68

4 meters

X3830A

X3830A

73 GB

73 GB

73 GB

DVD

HD68

HD68

HD68

HD68

D240

VHDCI-HD68

4 meters

X3830A

X3830A

73 GB

73 GB

73 GB

73 GB

HD68

HD68

HD68

HD68

D240

VHDCI-HD68

4 meters

X3830A

X3830A

Configuration Options

3120 SCSI Array

StorEdge 3120 SCSI Array

2, 3, or 4 Ultra320 SCSI Disks: 36GB 15K,

73GB 10K, 73GB 15K, 146GB 10K

Configurable to single or dual busses

Supports 1 or 2 hosts

N+1 Power & Fans

Dual power cords

1 Rack Units (1.75 in) high

JBOD only array

Can not be daisy chained

Not yet qualified as boot device

Rackmount Kit for Sun Rack 900 & Sun 72” Cabinet :

XTA-30001URK-19U

Sun Fire Cabinet support later.

Host Bus Adapters:

Cables:

X1138A

VHDCI-VHDCI

2 meters

X3830B

VHDCI-VHDCI

4 meters

X3831B

VHDCI-VHDCI

10 meters

X1136A

VHDCI-VHDCI

0.8 meter

X1137A

VHDCI-VHDCI

1.2 meters

6758A Dual LVD SCSI

VHDCI

VHDCI

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

2222A

10/100 Enet Dual RJ45's

LVD SCSI Dual VHDCI's

9265A U320 SCSI

VHDCI

VHDCI

V20z only

JBOD Array Configurations

Host

Host

1 Host, Single Bus

2 Host Connections, Dual Bus

2 Host Connections, Single Bus

Host

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3120

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3120

146 10k

146 10k

146 10k

146 10k

Host

Host

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3120

146 10k

146 10k

146 10k

146 10k

Disk Options

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

3310 SCSI Array

StorEdge 3310 SCSI Array

5-12 LVD SCSI Disks: 36GB 10K, 36GB 15K,

73GB 10K, 73GB 15K, 146GB 10K

5 TB raw disk total(RAID & 2 JBOD arrays)

Configurable to single or dual busses

N+1 Power & Fans

Dual power cords

2 Rack Units (3.5 in) high

RAID Array:

Up to 2 H/W Raid Controllers

512 MB cache for each controller

Built-in Battery

JBOD Array

Use as standalone or as expansion

to a RAID Array.

Raid Controllers can NOT be added to

JBOD Arrays

Rackmount Kit for Sun 72” Cabinet:

XTA-3310-RK-19L

Host Bus Adapter:

Cables:

X1138A

VHDCI-VHDCI

2 meters

X3830B

VHDCI-VHDCI

4 meters

X3831B

VHDCI-VHDCI

10 meters

X1136A

VHDCI-VHDCI

0.8 meter

X1137A

VHDCI-VHDCI

1.2 meters

6758A Dual LVD SCSI

VHDCI

VHDCI

146 10k

146 10k

146 10k

146 10k

Disk Options

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

JBOD Array Configurations

Host

Host

1 Host, Single Bus

2 Host Connections, Dual Bus

2 Host Connections, Single Bus

Host

Host

Host

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3310

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

73 10k

73 10k

73 10k

73 10k

73 10k

73 10k

73 10k

73 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3310

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3310

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

1 Host Connection, Dual Bus

RAID Array Configurations

Host

VHDCI Ch 0 Out

VHDCI Ch 3 I/O

VHDCI Dual Bus

VHDCI Sngle Bus

VHDCI Ch 1 I/O

VHDCI Ch 2 I/O

Space for RAID Controller

Space for RAID Controller

SE 3310

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

Terminator

XTA-3310-SC-TERM

1 or 2 Host Connections, Single Bus

Host

Host

VHDCI Ch 0 Out

VHDCI Ch 3 I/O

VHDCI Dual Bus

VHDCI Sngle Bus

VHDCI Ch 1 I/O

VHDCI Ch 2 I/O

Space for RAID Controller

Space for RAID Controller

SE 3310

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

RAID Array Sets

1 or 2 Host Connections

each array on separate Bus

2 Host Connections, Dual Bus

Host

Host

VHDCI Ch 0 Out

VHDCI Ch 3 I/O

VHDCI Dual Bus

VHDCI Sngle Bus

VHDCI Ch 1 I/O

VHDCI Ch 2 I/O

Space for RAID Controller

Space for RAID Controller

SE 3310

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

Host

Host

VHDCI Ch 0 Out

VHDCI Ch 3 I/O

VHDCI Dual Bus

VHDCI Sngle Bus

VHDCI Ch 1 I/O

VHDCI Ch 2 I/O

Space for RAID Controller

Space for RAID Controller

SE 3310

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3310

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

1 Host Connection

each array on separate Bus

Host

VHDCI Ch 0 Out

VHDCI Ch 3 I/O

VHDCI Dual Bus

VHDCI Sngle Bus

VHDCI Ch 1 I/O

VHDCI Ch 2 I/O

Space for RAID Controller

Space for RAID Controller

SE 3310

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

RAID Controller with 512 MB Cache

Serial DB9

Enet RJ45

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3310

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

VHDCI B Out

VHDCI B In

VHDCI A Out

VHDCI A In

SE 3310

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

3510 FC Array

StorEdge 3510 Fibre Channel Array

5x-12x 36, 73, or 146 GB FC Disks

5.1 TB max raw disk total (1 RAID &

2 JBOD Arrays)

N+1 Power & Fans

Dual power cords

2 Rack Units (3.5 in) high

RAID Array:

Up to 2 H/W Raid Controllers

1 GB cache for each controller

Built-in Battery Backup

JBOD Array:

Use as standalone or as expansion

to a RAID Array.

Raid Controllers can be added to

JBOD Arrays.

Rackmount Kit for 72” Cabinet:

XTA-3310-RK-19L

Host Bus Adapters:

Cables:

SFP:

XSFP-SW-2GB

JBOD Array Configurations

RAID Array Configuration

RAID Array Sets

Host 1

Host 2 (add a SPF)

4 single host connections or

2 redundant host connections

Host 1

Host 2 (add a SPF)

Dual RAID Controllers

8 single host connections or

4 redundant host connections

Single RAID Controller is supported

4 single host connections

Dual RAID Controller

8 single host connections or

4 redundant host connections

Dual JBOD Arrays

Single RAID Controller is supported

4 single host connections

Single JBOD Array is supported

X9732A

LC-LC fibre

2 meters

X9733A

LC-LC fibre

5 meters

X9734A

LC-LC fibre

15 meters

X9736A

LC-LC fibre

25 meters

X9738A

LC-LC fibre

50 meters

LC SFP

2 single host connections or

1 redundant host connection

SG-XPCI1FC-QF2 2Gb FC

LC

SG-XPCI2FC-QF2 2Gb FC

LC

LC

SE 3510

Loop A

Loop A

Loop B

Loop B

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

LC SFP

LC SFP

Host 1

Host 1

SE 3510

Loop A

Loop A

Loop B

Loop B

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

LC SFP

LC SFP

SE 3510

Space for

Controller

Space for

Controller

FC 0

FC 1

FC 2

FC 4

FC 5

RAID Controller

with 1 GB Cache

DB9 Serial

RJ45 Enet

FC 2

FC 0

FC 1

FC 3

FC 4

FC 5

RAID Controller

with 1 GB Cache

DB9 Serial

RJ45 Enet

FC 3

LC SFP

LC SFP

LC SFP

LC SFP

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

LC SFP

LC SFP

Host 3

Host 1

Host 4

Host 2

Host 1

Host 3 (add a SPF)

Host 2

Host 4 (add a SPF)

SE 3510

Space for

Controller

Space for

Controller

FC 0

FC 1

FC 2

FC 4

FC 5

RAID Controller

with 1 GB Cache

DB9 Serial

RJ45 Enet

FC 2

FC 0

FC 1

FC 3

FC 4

FC 5

RAID Controller

with 1 GB Cache

DB9 Serial

RJ45 Enet

FC 3

LC SFP

LC SFP

LC SFP

LC SFP

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

LC SFP

LC SFP

Host 3

Host 1

Host 4

Host 2

Host 1

Host 3

Host 2

Host 4

SE 3510

Loop A

Loop A

Loop B

Loop B

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

LC SFP

LC SFP

SE 3510

Loop A

Loop A

Loop B

Loop B

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

LC SFP

LC SFP

LC SFP

LC SFP

LC SFP

LC SFP

LC SFP

LC SFP

146 10k

146 10k

146 10k

146 10k

Disk Options

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

73 15k

73 10k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

73 10k

73 10k

73 10k

73 10k

73 10k

73 10k

73 10k

73 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

6120 FC Array

6120 Array Set

4 TB Disk, 2 GB cache

StorEdge 6120 Array

7-14 36, 73, or 146 GB FC Disks per tray

12 TB max raw disk total (2 RAID &

4 Expansion Trays)

N+1 Power & Fans

Dual power cords

3 Rack Units (3.5 in) high each tray

RAID Array:

H/W Raid Controller

1 GB cache

Built-in Battery Backup

Expansion Array:

Use as expansion to a RAID Array.

Raid Controllers can be added to

Expansion Arrays.

Rack Mount Kit:

X6886A 3 RU Rackmount Kit for Sun Rack 900,

72” Cabinet, and SunFire Cabinet:

Ships with:

5 meter LC-LC cable

6 meter RJ45-RJ45 Enet cable

Disk Options

7 to 14 disks per tray

Hot Spare

Location

73 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

36 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

73 15k

73 10k

146 10k

LC-LC fibre

5 meters

incl w/ 6120

LC-LC fibre

5 meters

incl w/ 6120

A

B

Space for RAID Controller

RJ45 Serial

RJ45 Enet

A

B

H/W RAID Controller

with 1 GB Cache

LC FC

A

B

Space for RAID Controller

RJ45 Serial

RJ45 Enet

A

B

H/W RAID Controller

with 1 GB Cache

LC FC

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

6320

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

Space for 6020 or 6120 tray

USB Ports

Serial

LAN

Service

Concentrator

Modem

Enet

Enet

Serial

Terminal

Concentrator

Service

USB Ports

650 MHz CPU

512 MB Memory

Storage Service

Processor

40 GB

16 Port

Switch

24 Port Enet Hub

5 Host Connections to top trays

Service Panel

16 Port

Switch

5 Host Connections to bottom trays

Expansion Rank

6320

22 6020 Trays

2 16-port 2GB Switches

1 Service Processor

45 TB

22 GB Cache

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

6020

6020

6020

6020

6020

6020

6020

6020

6020

6020

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

6020

6020

6020

6020

6020

6020

6020

6020

6020

6020

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

146

146

146

146

146

146

146

146

146

146

146

146

146 HS

146

Space for RAID Controller

RJ45 Serial

RJ45 Enet

H/W RAID Controller with 1 GB Cache

LC FC

A

B

6020

6020

24 Port Enet Hub

SE9970

SE 9970

2 GB Shared Memory

HDU

HDU

HDU

HDU

not functional

not functional

Crossbar Switch

11 GB

Cache

11 GB

Cache

4 Fiber Channel Ports

4 Fiber Channel Ports

Array

Control

Processor

Pair

Array

Control

Processor

Pair

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

Global hot spare disks:

Spare must be same size

and rpm as working disk.

36 GB 15k 73 GB 10k 73 GB 15k 146 GB 10k

36 15k

73 15k

73 10k

Available Disks:

146 10k

SE9970 Capacity:

128 Disks: 36/73/146 GB each

18 TB raw

32 GB cache

SE9980

Global hot spare disks:

Spare must be same size

and rpm as working disk.

36 GB 15k 73 GB 10k 73 GB 15k 146 GB 10k

36 15k

73 15k

73 10k

Available Disks:

146 10k

SE9980

Disk Controller Frame

Shared Memory: 3 GB

Crossbar Switch

L2 Disk Array Frame

HDU

HDU

HDU

HDU

HDU

HDU

HDU

HDU

L1 Disk Array Frame

HDU

HDU

HDU

HDU

HDU

HDU

HDU

HDU

R2 Disk Array Frame

HDU

HDU

HDU

HDU

HDU

HDU

HDU

HDU

R1 Disk Array Frame

HDU

HDU

HDU

HDU

HDU

HDU

HDU

HDU

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

4 Fiber Channel Ports

4 Fiber Channel Ports

4 Fiber Channel Ports

4 Fiber Channel Ports

4 Fiber Channel Ports

4 Fiber Channel Ports

4 Fiber Channel Ports

4 Fiber Channel Ports

Array

Control

Processor

Pair

Array

Control

Processor

Pair

Array

Control

Processor

Pair

Array

Control

Processor

Pair

Cache

16 GB

Cache

16 GB

Cache

16 GB

Cache

16 GB

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

146 10k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

73 15k

SE9980 Capacity:

1024 Disks: 36/73/146 GB each

147 TB raw

64 GB cache

Your Name Here

Your Email Address Here

2003-05-12T20:24:58