Sun StorEdge 9980

Full Configuration:

1024 x146GB/ 73 GB/ 36 GB Disks (149.5 TB / 74.7 TB / 36.8 TB raw)

16 of which can be global hot spares

8-64 Fiber Channel Host interfaces

6 GB Controller Memory

128 GB

System Controller Frame

4-port

FiChan

1 or 2Gb

8-port

FiChan

1 or 2 Gb

4-port

FICON

4-port

ESCON

4-port

FICON

4-port

ESCON

32-GB

cache

32-GB

cache

SE9900 Crossbar Switch

Array Frame L1

Array Frame L2

256MB

256MB

256MB

256MB

256MB

256MB

256MB

256MB

256MB

256MB

256MB

256MB

Shared Memory

32-GB

cache

32-GB

cache

1 x 146-GB (10k RPM) Spare AND / OR

1 x 73-GB (10k / 15K RPM) Spare AND / OR

1 x 36-GB (15k RPM) Spare (must be same speed as data disk)

8 or 4 146-GB (10k RPM)

8 or 4 x 73-GB (10k / 15k RPM)

8 or 4 x 36-GB (15k RPM) per RAID Group

Disk

Adaptor

Board

(DKA)

Pair

(Basic)

Disk

Adaptor

Board

(DKA)

Pair

(Add. 2)

Disk

Adaptor

Board

(DKA)

Pair

(Add. 1)

Disk

Adaptor

Board

(DKA)

Pair

(Add. 3)

Array Frame R1

Array Frame R2

4-port

FiChan

1 or 2Gb

8-port

FiChan

1 or 2 Gb

4-port

FICON

4-port

ESCON

Disk

Adaptor

Board

(DKA)

Pair

(Add. 2)

Disk

Adaptor

Board

(DKA)

Pair

(Add. 3)

4-port

FiChan

1 or 2Gb

8-port

FiChan

1 or 2 Gb

NAS

Blade

iSCSI

Blade

Site Plan

2 ft x 2 ft

Tile

Remote

Console

Keyboard

NEMA 5-15

100/120 VAC

15 amps

Sun Workstation

or Wintel PC

to run HiCommand

(Customer

Supplied)

NOTE: If three phase

is used, then power

for the controller

frame is supplied by

the disk frame.

Power

Single-Phase:

Power cords are

RussellStol 9P53U2

200/208/230 VAC

50 Amps

3-Phase 60Hz:

Power cords are

Russell Stol RS460PGW

200/208/230 VAC

30 Amp

Controller Cabinet

Dimensions:

31" (782mm) Width

31.5" (800mm) Depth

73" (1860mm)Height

0.6” (16mm) Side Cover

Clearances:

31.5" (800mm) Front

31.5 "(800mm) Back

Disk Array Frame

Dimensions:

29.5" (750mm) Width

31.5" (800mm) Depth

73" (1860mm)Height

0.6” (16mm) Side Cover

Clearances:

31.5" (800mm) Front

31.5 "(800mm) Back

Sun StorEdge

SE9980

Controller

Frame

Sun StorEdge

Disk

Array

Frame

Sun StorEdge

Disk

Array

Frame

Sun StorEdge

Disk

Array

Frame

Sun StorEdge

Disk

Array

Frame

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

1 / 2

1 / 2

SF15K Domain A

1 / 2

1 / 2

1 / 2

1 / 2

SF15K Domain B

1 / 2

1 / 2

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

Zone A

Zone A

Zone D

Zone B

Zone B

Zone C

Zone C

Zone D

Zone D

Zone A

Zone B

Zone C

32

GB

LC A

StorEdge 9980

32

GB

DKA

#4

DKA

#2

DKA

#1

DKA

#0

Disk Adapter Boards

Cache Memory

6 GB

Shared Memory

152

Active

Spindles

(4 spares)

152

Active

Spindles

(4 Spares)

Space

for

Disk

Frame

CHA

#1

CHA

#2

A LC

Space

for

Disk

Frame

LC B

LC C

LC D

LC E

LC F

LC G

LC H

LC J

LC K

LC L

LC M

B LC

C LC

D LC

E LC

F LC

G LC

H LC

J LC

K LC

L LC

M LC

32

GB

32

GB

Zone A

Zone B

Zone C

DR Target

LC N

LC P

LC R

LC S

Zone A

Zone B

Zone C

DR Initiator

N LC

P LC

R LC

S LC

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone D

SAN Zone A Connectivity Example / Template

SW-1

SW-2

SW-3

SW-4

COD

Prod

Adjust number of active spindles, spares, DKA, shared memory and cache

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

1 / 2

1 / 2

SF15K Domain 1

1 / 2

1 / 2

1 / 2

1 / 2

SF15K Domain 4

1 / 2

1 / 2

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

Zone A

Zone A

Zone D

Zone B

Zone B

Zone C

Zone C

Zone D

Zone D

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

DR Target

Zone A

Zone B

Zone C

DR Initiator

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone D

Production Test SAN Zone B Connectivity Example / Template

SW-1

SW-2

SW-3

SW-4

Test

Production ePay Failover

Adjust number of active spindles, spares, DKA, shared memory and cache

32

GB

LC A

StorEdge 9980

32

GB

DKA

#4

DKA

#2

DKA

#1

DKA

#0

Disk Adapter Boards

Cache Memory

6 GB

Shared Memory

152

Active

Spindles

(4 spares)

152

Active

Spindles

(4 Spares)

Space

for

Disk

Frame

CHA

#1

CHA

#2

A LC

Space

for

Disk

Frame

LC B

LC C

LC D

LC E

LC F

LC G

LC H

LC J

LC K

LC L

LC M

B LC

C LC

D LC

E LC

F LC

G LC

H LC

J LC

K LC

L LC

M LC

32

GB

32

GB

LC N

LC P

LC R

LC S

N LC

P LC

R LC

S LC

1 / 2

V210

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

1 / 2

1 / 2

V480

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

Zone A

Zone A

Zone D

Zone B

Zone B

Zone C

Zone C

Zone D

Zone D

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

DR Target

Zone A

Zone B

Zone C

DR Initiator

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone D

SAN Zone C Connectivity Example / Template

1 / 2

1 / 2

V480

1 / 2

1 / 2

V480

1 / 2

1 / 2

V480

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

1 / 2

V480

1 / 2

1 / 2

V480

1 / 2

1 / 2

V480

1 / 2

1 / 2

V480

DSS

CRM

Demo

Training

Messaging

Authentication

Development

SW-1

SW-2

SW-3

SW-4

Adjust number of active spindles, spares, DKA, shared memory and cache

32

GB

LC A

StorEdge 9980

32

GB

DKA

#4

DKA

#2

DKA

#1

DKA

#0

Disk Adapter Boards

Cache Memory

6 GB

Shared Memory

152

Active

Spindles

(4 spares)

152

Active

Spindles

(4 Spares)

Space

for

Disk

Frame

CHA

#1

CHA

#2

A LC

Space

for

Disk

Frame

LC B

LC C

LC D

LC E

LC F

LC G

LC H

LC J

LC K

LC L

LC M

B LC

C LC

D LC

E LC

F LC

G LC

H LC

J LC

K LC

L LC

M LC

32

GB

32

GB

LC N

LC P

LC R

LC S

N LC

P LC

R LC

S LC

1 / 2

V210

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

Zone A

Zone A

Zone D

Zone B

Zone B

Zone C

Zone C

Zone D

Zone D

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

DR Target

Zone A

Zone B

Zone C

DR Initiator

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone A

Zone B

Zone C

Zone D

SAN Zone D Connectivity Example / Template

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

LC

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

1 / 2

V210

SW-1

SW-2

SW-3

SW-4

SW-1

SW-2

SW-3

SW-4

SW-2

SW-4

Adjust number of active spindles, spares,

DKA, shared memory and cache

32

GB

LC A

StorEdge 9980

32

GB

DKA

#4

DKA

#2

DKA

#1

DKA

#0

Disk Adapter Boards

Cache Memory

6 GB

Shared Memory

152

Active

Spindles

(4 spares)

152

Active

Spindles

(4 Spares)

Space

for

Disk

Frame

CHA

#1

CHA

#2

A LC

Space

for

Disk

Frame

LC B

LC C

LC D

LC E

LC F

LC G

LC H

LC J

LC K

LC L

LC M

B LC

C LC

D LC

E LC

F LC

G LC

H LC

J LC

K LC

L LC

M LC

32

GB

32

GB

LC N

LC P

LC R

LC S

N LC

P LC

R LC

S LC

SE9980 Storage Array

SE9980

Jim Miller

2002-06-28T23:17:05

Edward Boyd

Elias Alagna