PC/SC SRCOM Bypass 2.0

This package enables the integrated Sun Ray smart card reader to be utilized
as a PC/SC compliant reader when used with 3rd party middleware products.
Personal Computer/Smart Card (PC/SC) is the standard framework for Smart 
Card device access on Windows, Linux and UNIX platforms. This library 
(binary) is a Sun Ray implementation of the PC/SC-lite API that is part of 
the Open Source MUSCLE project. This package requires Sun Ray Server 
Software (SRSS) 3.1 and

    - patch 120879-01 or later, for Solaris(sparc) systems.
    - patch 120880-01 or later, for Solaris(x86) systems.

The software operates in two modes. Single application mode and 
multi application mode.
By default, it installs in single application mode that lets
a single application access the reader.

To enable multiple applications accessing the reader simultaneously,
please run the script
      /opt/SUNWsrcbp/lib/utscconfig

To disable the feature of multiple applications accessing the reader
simultaneously, please run the unconfiguration script,
      /opt/SUNWsrcbp/lib/utscconfig -u

Please send your Questions/Comments to: sunray-pcsc-ext@sun.com
