Volume Servers

B1600 Blades

Chassis with 16 Blade Servers

Administration Tools

V210 Server

2 USIIIi CPU's - 1 GHz

8 GB memory

2 internal 36 GB disks

V240 Server

2 USIIIi CPU's - 1.28 GHz

8 GB memory

4 internal 36 GB disks

V440 Server

4 USIIIi CPU's – 1.28 GHz

16 GB memory

4 internal 36 GB Disks

V250 Server

2 USIIIi CPU's - 1.28 GHz

8 GB memory

8 internal 73 GB Disks

Volume Servers

V880 Server

8 USIII CPU's - 1.2 GHz

64 GB memory

12 internal 146 GB disks

V480 Server

4 USIII CPU's – 1.2 GHz

32 GB memory

2 internal 73 GB Disks

280R Server

2 USIII CPU's - 1.2 GHz

8 GB memory

2 internal 36 GB Disks

V490 Server

4 USIV CPU's – 1.05 GHz

32 GB memory

2 internal 73 GB Disks

V890 Server

8 USIV CPU's - 1.2 GHz

64 GB memory

12 internal 146 GB disks

Volume Servers - x86 Servers

V60x Server

2 Intel CPU's - 2.8 or 3.2 GHz

6 GB memory

3 internal 73 GB disks

Solaris x86 or Linux

V65x Server

2 Intel CPU's - 3.2 GHz

12 GB memory

6 internal 73 GB disks

Solaris x86 or Linux

V20z Server

2 AMD Opteron CPU's - 1.6, 1.8 or 2.2 GHz

16 GB memory

2 internal 73 GB disks

Solaris x86 or Linux

Sun Rack 900

Volume Servers

V880 Server

8 CPU's, 12 Disks

V480 Server

4 CPU's, 2 Disks

V280 Server

2 CPU's, 2 Disks

V210 Server

2 CPU's, 2 Disks

V240 Server

2 CPU's, 4 Disks

The V880 needs a

rack specific mount

kit.

V20z is not

supported in this

cabinet.

Sun 72” Cabinet

V60x Server

2 CPU's, 2 Disks

V65x Server

2 CPU's, 6 Disks

V880

V880 Rack Mount Kit

Sun Rack 900

V480

V210

V280

V240

V60x

V65x

B1600 Blades

16 Blade Servers

B1600

V440

V440 Server

4 CPU's, 4 Disks

V20z

V20z Server

2 CPU's, 2 Disks

V100 Server

1 CPU, 1 Disk

V120 Server

1 CPU, 1 Disk

V120

V100

V890 Server

8 CPU's, 12 Disks

V490 Server

4 CPU's, 2 Disks

V6

V880 Rack Mount Kit

Sun Rack 900

V490

SPARC

Sun Fire B1600 Detail

Sun Fire B1600

Integrated Switches &System Controller

Redundant Power, 3 RU Chassis

Ships with:

Rack Mount Kit for Sun Rack 900

& Sun 72” Cabinet

Content Load Balancing

B10n

1.5

GHz

AMD

30

GB

Disk

1 GB

B100x

SSL Proxy Blade

B10p

x86

Specialty

I2C

5

DC

Midplane

Switch

System

Controller

10/100/1000 Cat-5 Enet RJ45

LOM Serial Port RJ45

10/100 System Mgmt Link RJ45

16

GBE

2

SC-SC

Link

16

Serial

Mgmt

Link

5

I2C

Switch

System

Controller

LOM Serial Port RJ45

10/100 System Mgmt Link RJ45

16

GBE

2

SC-SC

Link

16

Serial

Mgmt

Link

5

I2C

PSU

Power

I2C

5

DC

PSU

Power

Sun Fire

B1600

Chassis

Space

for

Blade

Gbe

Gbe

Serial

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

Space

for

Blade

Gbe

Gbe

Serial

1.5

GHz

AMD

30

GB

Disk

2 GB

B100x

30

GB

Disk

1 GB

B200x

1 GB

2.0

GHz

Intel

2.0

GHz

Intel

30

GB

Disk

1 GB

B200x

1 GB

2.0

GHz

Intel

2.0

GHz

Intel

30

GB

Disk

512

MB

B100s

650

MHz

USII

30

GB

Disk

1

GB

B100s

650

MHz

USII

30

GB

Disk

2

GB

B100s

650

MHz

USII

V100

1 USII CPU - 650 or 550 MHz

1 GB memory (4 GB Max)

2 internal disks (IDE) - 80 GB each

CD-ROM

1 Rack Unit High (1.75 in.)

Included Rack Mount Kit fits:

Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

V100 Server Detail

V100

USB

Serial

Power

CDROM

Space for Memory

10/100 Enet

Space for Memory

10/100 Enet

Serial

650 MHz

USII

System Config Card

Space for Memory

Space for Memory

Space

for Disk

Space

for Disk

80 GB

Disk

512 MB memory

512 MB memory

80 GB

Disk

V120 Server Detail

V120

1 USII CPU - 650 MHz

512 MB memory (4 GB max)

73 GB internal SCSI disk (2 max)

Slot for CD-ROM or DVD

33 MHz PCI slot

1 Rack Unit High (1.75 in.)

Included Rack Mount Kit fits

Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

V120

USB

Power

650 MHz

USII

Space for Memory

Space for Memory

10/100 Enet RJ45

Serial DB9

Space for

CDROM

or DVD

UltraSCSI HD68

33 MHz PCI Slot

System Config Card

10/100 Enet RJ45

Serial DB9

Space

for Disk

Space for Memory

Space for Memory

Space

for Disk

73 GB

Disk

73 GB

Disk

256 MB memory

256 MB memory

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

V210 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

ALOM

Space for Sun Crypto

Accelerator 500

Space

for

CPU

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Space

for Disk

Space

for Disk

V210 Server Detail

V210 Server

Capacity:

2 USIIIi CPU's - 1.06 GHz each

8 GB memory

2 internal 36 or 73 GB LVD disks

1 PCI Slot - 66 MHz

4 10/100/1000Base -T Ethernet Ports

DVD Drive Option

Sun Crypto Accelerator Card Option

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Single Power Supply.

Single Power Cord

1 Rack Unit high

Ships with:

Rack Mounting with cable management

fits Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

System Key

RJ-45 to DB-9 Adapter

RJ-45 to DB-25 Adapter

Cat5 RJ-45 cable

2 CPU, 2 GB memory, 2x 36 GB disk, base configuration

1 CPU, 512 MB memory, 1x 36 GB disk, base configuration

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

V210 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

ALOM

Space for Sun Crypto

Accelerator 500

Space

for

CPU

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space

for

CPU

Space

for Disk

Space

for Disk

36 GB

Disk

512 MB

1.06

GHz

USIIIi

36 GB

Disk

36 GB

Disk

1.06

GHz

USIIIi

1.06

GHz

USIIIi

1 GB

1 GB

Disk Options

36 GB

Disk

73 GB

Disk

DVD

DVD Option

Memory Options

1 GB

2 GB

512 MB

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

System Config Card

33 MHz PCI Slot

33 MHz PCI Slot

Power Supply

Power

V240 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

ALOM

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space for Sun Crypto

Accelerator 500

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

66 MHz PCI Slot

Space for

DVD drive

Power Supply

Power

USB

System Config Card

33 MHz PCI Slot

33 MHz PCI Slot

Power Supply

Power

V240 Server

LVD SCSI VHDCI

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Serial Port DB9

ALOM

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

Space for Sun Crypto

Accelerator 500

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

V240 Server Detail

V240 Server

Capacity:

2 USIIIi CPU's - 1.06 or 1.28 GHz each

8 GB memory

4 internal 36 or 73 GB LVD disks

3 PCI Slots - 1x 66 MHz, 2x 33 MHz

4 10/100/1000Base -T Ethernet Ports

DVD Drive Option

Sun Crypto Accelerator Card Option

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Redundant Power Supplies.

2 Power Cords

2 Rack Units high

Ships with:

Rack Mounting with cable management

fits Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

System Key

RJ-45 to DB-9 Adapter

RJ-45 to DB-25 Adapter

Cat5 RJ-45 cable

2 CPU, 8 GB memory, 2x 36 GB disk, base configuration

1 CPU, 512 MB memory, 1x 36 GB disk, base configuration

Disk Options

36 GB

Disk

73 GB

Disk

DVD

DVD Option

Memory Options

1 GB

2 GB

1.06

GHz

USIIIi

512 MB

36 GB

Disk

1.28

GHz

USIIIi

1.28

GHz

USIIIi

2 GB

2 GB

2 GB

2 GB

36 GB

Disk

36 GB

Disk

512 MB

V250 Server Detail

V250 Server

Capacity:

2 USIIIi CPU's - 1.06 or 1.28 GHz each

8 GB memory (4 GB per CPU)

8 internal 36 or 73 GB Ultra160 SCSI disks

6 PCI Cards - 3x 66/33 MHz, 3x 33 MHz

1 10/100/1000Base -T Ethernet Port

DVD Drive

Optional DDS4- DAT tape drive

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Redundant Power Supplies.

2 Power Cords

1 CPU, 512 MB memory, 1x 36 GB disk, base configuration

2 CPU's, 8 GB memory, 2x 73 GB disk, base configuration

Disk Options

DDS-4 Tape

Tape Option

Memory Options

1 GB

2 GB

36 GB Disk

73 GB Disk

Space for

DAT tape

Power

2x USB 1.0

LVD SCSI VHDCI

Serial Port RJ45

10/100/1000 Cat-5 Enet RJ45

10/100 Enet RJ45

System Config Card

Serial Port DB9

ALOM

V250 Server

Parallel Port DB25

2x USB 1.0

DVD drive

Power Supply

Power

Power Supply

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space

for

CPU

Space

for

CPU

Space for

Disk

1.06

GHz

USIIIi

512 MB

36 GB Disk

Space for

DAT tape

Power

2x USB 1.0

LVD SCSI VHDCI

Serial Port RJ45

10/100/1000 Cat-5 Enet RJ45

10/100 Enet RJ45

System Config Card

Serial Port DB9

ALOM

V250 Server

Parallel Port DB25

2x USB 1.0

DVD drive

Power Supply

Power

Power Supply

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space

for

CPU

Space

for

CPU

Space for

Disk

1.28

GHz

USIIIi

1.28

GHz

USIIIi

2 GB

2 GB

2 GB

2 GB

73 GB Disk

73 GB Disk

512 MB

280R Server Detail

280R Server

2 USIII CPU's - 1.2 GHz

4 GB memory (8 GB max)

2 internal 36 disks

4 PCI Cards - 1x 66 MHz, 3x 33 MHz

DVD Drive

N+1 Power & Fans.

Dual Power Cords

4 Rack Units (7 in.) high

Included Rack Mount Kit fits

Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

66 MHz PCI Slot

33 MHz PCI Slot

Space for Memory

DVD drive

Serial A / B

56k modem

Remote System

Control

10 Ethernet

Power Supply

Power

Power Supply

Power

USB

280R Server

UltraSCSI HD68

Space for

CPU

10/100 Enet RJ45

Serial A/B DB27

33 MHz PCI Slot

33 MHz PCI Slot

Space

for Disk

Space

for Disk

Space for

CPU

Space for Memory

1.2 GHz

USIII

1.2 GHz

USIII

2 GB memory

2 GB memory

36 GB

Disk

36 GB

Disk

V440 Server Detail

4 CPU's, 16 GB memory, 4 x 73 GB disk, base configuration

V440 Server

Capacity:

4 USIIIi CPU's - 1.062 or 1.28 GHz each

16 GB memory (4 GB per CPU)

4 internal 36 or 73 GB Ultra320 SCSI disks

6 PCI Cards - 3x 66/33 MHz, 3x 33 MHz

2 10/100/1000Base -T Ethernet Ports

DVD Drive

Advanced Lights Out Management (ALOM) Card

System Configuration Card

Redundant Power Supplies.

2 Power Cords

4 Rack Units high

Ships with:

Rack Mounting with cable management

fits Sun 900 Rack, Sun 72” Cab, Sun Fire Cab

System Key

RJ-45 to DB-9 Adapter

RJ-45 to DB-25 Adapter

Cat5 RJ-45 cable

Disk Options

36 GB

Disk

DVD drive

Power Supply

Power

V440 Server

Ultra320 SCSI HD68

Serial Port RJ45

10/100 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

System Config Card

Serial Port DB9

Power Supply

Power

ALOM

USB

USB

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

Space for

CPU / Mem

Board

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

66 MHz PCI Slot

66 MHz PCI Slot

Space

for Disk

Space

for Disk

Space

for Disk

Space

for Disk

33

66

33

66

33

66

73 GB

Disk

73 GB

Disk

73 GB

Disk

73 GB

Disk

2 GB

1.28

GHz

USIIIi

2 GB

2 GB

1.28

GHz

USIIIi

2 GB

2 GB

1.28

GHz

USIIIi

2 GB

2 GB

1.28

GHz

USIIIi

2 GB

73 GB

Disk

V480 Server Detail

V480 Server

4 USIII CPU's – 1.2 GHz

32 GB memory

2 internal 73 GB FCAL disks

DVD

6 PCI Cards - 2x 66 MHz, 4x 33 MHz

2x 10/100/1000 Cat-5 Ethernet

N+1 Power & Fans.

Dual Power Cords

5 Rack Units (8.75 in.) high

Included Rack Mount Kit fits

Sun 900 Rack & Sun 72” Cabinet

V480

Space

for

CPU / Memory

Board

Power Supply

USB

Serial RJ45

Power

Power Supply

Power

Space

for

CPU / Memory

Board

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33

66

66

33

33

33

System Controller

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

DVD

space for disk

73 GB Disk

space for disk

73 GB Disk

Serial RJ45

Enet RJ45

Modem RJ11

33 MHz PCI Slot

66 MHz PCI Slot

V490 Server Detail

V490

Space

for

CPU / Memory

Board

Power Supply

USB

Serial RJ45

Power

Power Supply

Power

Space

for

CPU / Memory

Board

10/100/1000 Cat-5 Enet RJ45

10/100/1000 Cat-5 Enet RJ45

33

66

66

33

33

33

1.05 GHz

USIV

1.05 GHz

USIV

2 GB

2 GB

2 GB

2 GB

1.05 GHz

USIV

1.05 GHz

USIV

2 GB

2 GB

2 GB

2 GB

DVD

space for disk

73 GB Disk

space for disk

73 GB Disk

33 MHz PCI Slot

66 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

System Controller

Serial RJ45

Enet RJ45

66 MHz PCI Slot

V490 Server

4 USIV CPU's – 1.05 GHz

32 GB memory

2 internal 73 or 146 GB FCAL disks

DVD

6 PCI Cards - 2x 66 MHz, 4x 33 MHz

2x 10/100/1000 Cat-5 Ethernet

N+1 Power & Fans.

Dual Power Cords

5 Rack Units (8.75 in.) high

Included Rack Mount Kit fits

Sun 900 Rack & Sun 72” Cabinet

V880 Server Detail

V880 Server

8 USIII CPU's - 1.2 GHz

16 GB memory (64 GB max)

6 internal 73 GB FCAL disks (12 max)

DVD

9 PCI Cards - 2x 66 MHz, 7x 33 MHz

10/100 Enet

Fiber 1000 Enet

N+1 Power & Fans.

3 Power Cords

17 Rack Units high

X9638A Sun 900 Rack Mount Kit

X9628A Sun 72” Cabinet Mount Kit

X6756A

Second Backplane

with 6x 73 GB Disks

Second Backplane

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

73

GB

73

GB

73

GB

73

GB

73

GB

73

GB

Second Backplane

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

146

GB

146

GB

146

GB

146

GB

146

GB

146

GB

X6858A

Second Backplane

with 6x 146 GB Disks

66 MHz PCI Slot

66 MHz PCI Slot

Space for Disk Backplane

33 MHz PCI Slot

DVD

Space for Tape

Space

for

CPU / Memory

Board

Internal IDE

Space

for

CPU / Memory

Board

Space for Tape

73

GB

73

GB

73

GB

73

GB

73

GB

73

GB

Power Supply

Power

USB

Serial

Power Supply

Power

Power Supply

Power

Space

for

CPU / Memory

Board

Space

for

CPU / Memory

Board

10/100 Enet RJ45

Gb Enet SC

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Serial A/B

33

66

66

33

33

33

33

33

33

66

System Controller

Serial RJ45

Enet RJ45

Modem RJ11

V880

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

1.2 GHz

USIII

1.2 GHz

USIII

1 GB

1 GB

1 GB

1 GB

Internal Cable

X6755A

6727A Dual Gb FC

SC

SC

V890 Server Detail

X6756A

Second Backplane

with 6x 73 GB Disks

Second Backplane

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

73

GB

73

GB

73

GB

73

GB

73

GB

73

GB

Second Backplane

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

Space

for

Disk

146

GB

146

GB

146

GB

146

GB

146

GB

146

GB

X6858A

Second Backplane

with 6x 146 GB Disks

66 MHz PCI Slot

66 MHz PCI Slot

Space for Disk Backplane

33 MHz PCI Slot

DVD

Space for Tape

Space

for

CPU / Memory

Board

Internal IDE

Space

for

CPU / Memory

Board

Space for Tape

73

GB

73

GB

73

GB

73

GB

73

GB

73

GB

Power Supply

Power

USB

Serial

Power Supply

Power

Power Supply

Power

Space

for

CPU / Memory

Board

Space

for

CPU / Memory

Board

10/100 Enet RJ45

Gb Enet SC

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

33 MHz PCI Slot

Serial A/B

33

66

66

33

33

33

33

33

33

66

V890

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

Internal Cable

X6755A

6727A Dual Gb FC

SC

SC

System Controller

Serial RJ45

Enet RJ45

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

1.2 GHz

USIV

1.2 GHz

USIV

2 GB

2 GB

2 GB

2 GB

V890 Server

8 USIV CPU's - 1.2 GHz

32 GB memory (64 GB max)

6 internal 73 GB FCAL disks (12 max)

DVD

9 PCI Cards - 2x 66 MHz, 7x 33 MHz

10/100 Enet

Fiber 1000 Enet

N+1 Power & Fans.

3 Power Cords

17 Rack Units high

X9638A Sun 900 Rack Mount Kit

X9628A Sun 72” Cabinet Mount Kit

V20z Server Detail

V20z Server

Capacity:

1 or 2 AMD Opteron CPU's - 1.6, 1.8 or 2.2 GHz

1 - 16 GB memory

1-2 internal U320 SCSI (36/73) disk drives

CD + Floppy Drive

2 PCI-X Card Slots - 133/66 MHz

1 Full-Size 133/66 MHz , 1 Low Profile 66 MHz

2 10/100/1000 BaseT Ethernet Ports

1 USB port

PS/2 keyboard / mouse support

IPMI System Processor

1 power cord

1 Rack Unit high

X9267A Rack Mount Kit for Sun Rack 900

Not Supported in 72” Cabinet

Ships with:

Linux Resource CD (drivers, IPMI utils, etc.)

1x 1.6 MHz CPU, 1 GB memory, 1x 36 GB disk configuration

2x 2.2 GHz CPU's, 4 GB memory, 2x 36 GB disk configuration

DVD + Floppy

Flex Bay Options

Disk Options

9265A U320 SCSI

VHDCI

VHDCI

Memory

1 GB

2 GB

9271A 1000/100/10 Enet

RJ45

9272A 1000/100/10 Enet

RJ45

RJ45

9273A Quad 1000/100 Enet RJ45's

4 GB

133 MHz Only

Full Size Only

9279A 2 Gb FC-AL

LC

PCI-X Cards

Low Profile (also fits Full Size Slot)

36 GB

Disk

USB

V20z Server

Serial Port DB9

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

Keyboard PS/2

Full size 133/66 MHz PCI-X Slot

Video DB15

CD + Floppy

Flex Bay

Low Profile 66 MHz PCI-X slot

Mouse PS/2

10/100 Enet RJ45

10/100 Enet RJ45

IPMI

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

1 GB

36 GB

Disk

1.6 GHz

Opteron

CPU

USB

V20z Server

Serial Port DB9

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

Keyboard PS/2

Full size 133/66 MHz PCI-X Slot

Video DB15

CD + Floppy

Flex Bay

Low Profile 66 MHz PCI-X slot

Mouse PS/2

10/100 Enet RJ45

10/100 Enet RJ45

IPMI

Space

for

CPU

Space

for

CPU

Space

for Disk

Space

for Disk

36 GB

Disk

2.2 GHz

Opteron

CPU

2.2 GHz

Opteron

CPU

2 GB

2 GB

73 GB

Disk

146 GB

Disk

V60x Server Detail

V60x Server

Capacity:

1 or 2 Intel Xeon 2.8 or 3.2 GHz CPU's

512MB- 6 GB memory

1-3 internal U-320 LVD (36/73/146) disk drives

CD + Floppy Drive

2 PCI-X Card Slots - 100/66/33 MHz

1 Full-Size, 1 Low-Profile PCI

2 10/100/1000 BaseT Ethernet Ports

3 USB ports

PS/2 keyboard / mouse support

Graphics support up to 1600 x 1200

IPMI for remote management

1 power cord

1 Rack Unit high

X5030A Rack Mount Kit for Sun Rack 900 & 72” Cabinet

X5137A Serial & RJ45 dongle kit

Ships with:

Linux Resource CD (drivers, IPMI utils, etc.)

PS/2 "Y" splitter

1x 2.8 GHz CPU, 512 MB memory, 1x 36 GB disk configuration

2x 3.2 GHz CPU's, 2 GB memory, 2x 36 GB disk configuration

DVD + Floppy

Flex Bay Options

Disk Options

PCI Card Options

5132A RAID Controller

5133A 1 Gb FC

SC

Memory Options

256 MB memory

256 MB memory

512 MB memory

512 MB memory

1 GB memory

1 GB memory

USB

V60x Server

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

DB15 Video

Keyboard & Mouse

100/66/33 MHz PCI-X Slot

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

CD + Floppy

Flex Bay

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

Low Profile PCI-X Slot

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

3.2 GHz

Xeon

CPU

1 GB memory

1 GB memory

3.2 GHz

Xeon

CPU

36 GB

Disk

USB

V60x Server

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Power Supply

Power

DB15 Video

Keyboard & Mouse

100/66/33 MHz PCI-X Slot

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

CD + Floppy

Flex Bay

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

Low Profile PCI-X Slot

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

36 GB

Disk

256 MB memory

256 MB memory

2.8 GHz

Xeon

CPU

36 GB

Disk

73 GB

Disk

36 GB

Disk

73 GB

Disk

36 GB

Disk

146 GB

Disk

V65x Server Detail

1x 2.8 GHz CPU, 512 GB memory, 1x 36 GB disk configuration

V65x Server

Capacity:

1 or 2 Intel Xeon CPU's, 2.8 GHz or 3.2 GHz

512MB- 12 GB memory

1-6 internal U-320 LVD (36/73/146) disk drives

CD + Floppy Drive

6 PCI-X Cards - 100/66/33 MHz

3 Full-size PCI slots, 3 Low-profile slots

2 10/100/1000 BaseT Ethernet Ports

3 USB ports

PS/2 keyboard / mouse support

Graphics support up to 1600 x 1200

IPMI for remote management

Redundant Power Supply Option.

1 Power Cords per Power Supply

2 Rack Units high

X5030A Rack Mount Kit for Sun Rack 900 & 72” Cabinet

X5137A Serial & RJ45 dongle kit

Ships with:

Linux Resource CD (drivers, IPMI utils, etc.)

PS/2 "Y" splitter

DVD + Floppy

36 GB

Disk

73 GB

Disk

2x 3.2 GHz CPU, 1 GB memory, 1x 36 GB disk configuration

Power

2nd Power Supply

5132A RAID Controller

Flex Bay Options

Disk Options

PCI Card Options

Memory Options

256 MB memory

256 MB memory

512 MB memory

512 MB memory

1 GB memory

1 GB memory

2 GB memory

2 GB memory

Redundant Power Option

5133A 1 Gb FC

SC

USB

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Space for Power Supply

DB15 Video

Keyboard & Mouse

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

Power Supply

Power

V65x Server

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

Low Profile PCI-X Slot

Flex Bay

CD + Floppy

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

Low Profile PCI-X Slot

Low Profile PCI-X Slot

3.2 GHz

Xeon

CPU

512 MB memory

512 MB memory

3.2 GHz

Xeon

CPU

36 GB

Disk

USB

LVD SCSI VHDCI

ISC Serial Port RJ45

10/100/1000 Cat-5 RJ45

10/100/1000 Cat-5 RJ45

Space for Power Supply

DB15 Video

Keyboard & Mouse

Internal SCSI

USB

ATI Rage w/ 8MB

Video DB15

USB

Power Supply

Power

V65x Server

Space for

CPU

Space for memory

Space for memory

Space for memory

Space for memory

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

100/66/33 MHz PCI-X Slot

Low Profile PCI-X Slot

Flex Bay

CD + Floppy

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for

Disk

Space for memory

Space for memory

Space for

CPU

Low Profile PCI-X Slot

Low Profile PCI-X Slot

36 GB

Disk

256 MB memory

256 MB memory

2.8 GHz

Xeon

CPU

146 GB

Disk

SCSI Cables

X979A

X973A

SC-SC fibre

2 meters

X978A

HD68 - HD68

SC - SC Fibre

X9715A

VHDCI - HD68

VHDCI - VHDCI

Fibre Cables

SC - LC Fibre

LC / LC Fibre

X1138A

VHDCI-VHDCI

2 meters

X3830B

VHDCI-VHDCI

4 meters

X3831B

VHDCI-VHDCI

10 meters

X1136A

VHDCI-VHDCI

0.8 meter

X3810A

X1132A

VHDCI-HD68

0.8 meter

X1134A

HD68-HD68

0.8 meter

X1139A

HD68-HD68

2 meters

HD68-HD68

4 meters

HD68-HD68

12 meters

X3832A

VHDCI-HD68

2 meters

X3830A

VHDCI-HD68

4 meters

X3831A

VHDCI-HD68

10 meters

SC-SC fibre

5 meters

SC-SC fibre

15 meters

X9722A

SC-LC fibre

2 meters

X9721A

SC-LC fibre

0.4 meter

X9723A

SC-LC fibre

5 meters

X9724A

SC-LC fibre

15 meters

X9735A

SC-LC fibre

25 meters

X9737A

SC-LC fibre

50 meters

X9732A

LC-LC fibre

2 meters

X9733A

LC-LC fibre

5 meters

X9734A

LC-LC fibre

15 meters

X9736A

LC-LC fibre

25 meters

X9738A

LC-LC fibre

50 meters

X1137A

VHDCI-VHDCI

1.2 meters

66/33 MHz PCI Cards

33 MHz PCI Cards

PCI Cards

1155A High Speed Serial 2.0

1071A HIPPI/P 1.1

2156A Serial Async 3.0

6799A Gb FC

SC

6727A Dual Gb FC

SC

SC

SG-XPCI1FC-QF2 2Gb FC

LC

SG-XPCI2FC-QF2 2Gb FC

LC

LC

6758A Dual LVD SCSI

VHDCI

VHDCI

4422A

10/100/1000 Enet RJ45's

SE/LVD SCSI VHDCI's

6540A UltraSCSI

VHDCI

VHDCI

6541A UltraSCSI Diff

VHDCI

VHDCI

1157A ATM 155 4.0

MMF

X9739A

SC-SC fibre

100 meters

Was 6767A

Was 6768A

SG-XPCI1FC-JF2 JNI 2Gb

LC

3151A Gb Enet

MMF

3150A 1000/100/10 Enet

RJ45

SG-XPCI2FC-JF2 JNI 2Gb

LC

LC

1074A SCI cluster

Full Length: does not fit into V2900/V1280

4444A 10/100/1000 Enet RJ45's

PCI Cards & Cables

Site Plan

2 ft x 2 ft

Tile

72" Cabinet

Power cords are

NEMA #L6-30P

200/240 VAC

Single Phase

24 amps each

72" Cabinet

24" Width

37" Depth

73.7" Height

Clearances:

48" Front

36" Back

Sun Rack 900

Power cords are

NEMA L6-20P

200/240 VAC

Single Phase

16 amps each

Sun Rack 900

23.5" Width

35.4" Depth

74" Height

Clearances:

48" Front

36" Back

Power Distribution Sys:

12 outlets per external

power cord

20 internal cords included

24 outlets

24 outlets

9 outlets

9 outlets

11 connects:

7 reg cords

2 split cords

11 connects:

7 reg cords

2 split cords

Front Door Option

Front Door Option

Tom Meier

2000-03-25T11:55:10